IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
File name: "0001"
Time stamp: "2015-05-08T13:45:19"
Preprocessor: "The EXPRESS Data Manager Version 5.01.0100.02.64mod : 6 Jun 2012"
Originating system: "20130308_1515(x64) - Exporter 2014.0.2013.0308 - Default UI"
Application: "Autodesk Revit 2014 (ENU)" version "2014" identifier "Revit" by Organization "Autodesk Revit 2014 (ENU)"

People and organizations
  Person "BTN" of Organization (no name given)
  Owner history of Person "BTN" of Organization (no name given) | application "Autodesk Revit 2014 (ENU)" version "2014" identifier "Revit" by Organization "Autodesk Revit 2014 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: KELVIN
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  POWERUNIT: WATT

Spatial structure
IFCPROJECT "0001" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 30.344238″ | longitude -71° 3′ 35.194702″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "<Default>"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 9 elements
          1 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "Condensing-Storage-Water-Heater-Gas-AO_Smith-TWI-45-190_PG" | object type "Condensing-Storage-Water-Heater-Gas-AO_Smith-TWI-45-190_PG" | names: "Condensing-Storage-Water-Heater-Gas-AO_Smith-TWI-45-190_PG:Condensing-Storage-Water-Heater-Gas-AO_Smith-TWI-45-190_PG:708216" | material: "Workspace 3D" | property sets: Mechanical, Constraints, Identity Data, Other, Phasing, Pset_ManufacturerTypeInformation
          1 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "10.Boiler TWI" | object type "10.Boiler TWI" | names: "01. Boiler TWI-45:10.Boiler TWI:708218" | material: materials ("RAL 9005", "RAL 9006") | property sets: Constraints, Phasing, Identity Data
          1 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "01.Chimney Pipe" | object type "01.Chimney Pipe" | names: "02. Chimney Pipe:01.Chimney Pipe:708220" | material: materials ("Aluminium") | property sets: Constraints, Identity Data, Phasing
          1 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "09.Control panel TWI" | object type "09.Control panel TWI" | names: "09.Control panel TWI:09.Control panel TWI:708221" | material: materials ("RAL 9005", "Aluminium", "Green light", "Yellow light", "Red light", "Twister - Control panel") | property sets: Constraints, Phasing, Identity Data
          2 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "08.Cover plate 2" | object type "08.Cover plate 2" | names: "05. Cover plate:08.Cover plate 2:708222", "05. Cover plate:08.Cover plate 2:708223" | material: "RAL 9005" | property sets: Identity Data, Constraints, Phasing
          1 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "03.Gas control (external)" | object type "03.Gas control (external)" | names: "05.Gas control (external):03.Gas control (external):708225" | material: materials ("Aluminium", "RAL 9005") | property sets: Identity Data, Constraints, Phasing
          1 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "01. Water control (external)" | object type "01. Water control (external)" | names: "04. Water control (external):01. Water control (external):708227" | material: materials ("Rubber", "Aluminium") | property sets: Identity Data, Constraints, Phasing
          1 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "01. Water control (external)" | object type "01. Water control (external)" | names: "04. Water control (external):01. Water control (external):708228" | material: materials ("Rubber", "Aluminium") | property sets: Identity Data, Constraints, Phasing

Types
  IFCBOILERTYPE "Condensing-Storage-Water-Heater-Gas-AO_Smith-TWI-45-190_PG" | element type "Condensing-Storage-Water-Heater-Gas-AO_Smith-TWI-45-190_PG" | 1 occurrence | material: "Workspace 3D"
  IFCBOILERTYPE "10.Boiler TWI" | element type "10.Boiler TWI" | 1 occurrence | material: materials ("RAL 9005", "RAL 9006")
  IFCBOILERTYPE "01.Chimney Pipe" | element type "01.Chimney Pipe" | 1 occurrence | material: materials ("Aluminium")
  IFCBOILERTYPE "09.Control panel TWI" | element type "09.Control panel TWI" | 1 occurrence | material: materials ("RAL 9005", "Aluminium", "Green light", "Yellow light", "Red light", "Twister - Control panel")
  IFCBOILERTYPE "08.Cover plate 2" | element type "08.Cover plate 2" | 2 occurrences | material: "RAL 9005"
  IFCBOILERTYPE "03.Gas control (external)" | element type "03.Gas control (external)" | 1 occurrence | material: materials ("Aluminium", "RAL 9005")
  IFCBOILERTYPE "01. Water control (external)" | element type "01. Water control (external)" | 1 occurrence | material: materials ("Rubber", "Aluminium")
  IFCBOILERTYPE "01. Water control (external)" | element type "01. Water control (external)" | 1 occurrence | material: materials ("Rubber", "Aluminium")

Property sets
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Constraints | properties | on 4 objects (4 IFCENERGYCONVERSIONDEVICE)
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 2 objects (2 IFCENERGYCONVERSIONDEVICE)
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 30. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 100. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 1.11311663148492 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Mechanical | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    System Classification = "Domestic Hot Water,Domestic Cold Water,Other,Vent" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    APS Pressure < = 131.064 (IFCREAL)
  Identity Data | properties | on 8 objects (8 IFCENERGYCONVERSIONDEVICE)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Mark = "1" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Mark = "2" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Mark = "4" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Mark = "5" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Mark = "6" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Mark = "7" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Mark = "9" (IFCTEXT)
  Identity Data: 5 more contents on 5 objects not shown
  Other | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Workspace = TRUE (IFCBOOLEAN)
  Other | properties | on 1 object (1 IFCBUILDING)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "0001" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Phasing | properties | on 9 objects (9 IFCENERGYCONVERSIONDEVICE)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Manufacturer = "A.O. Smith Water Products Company b.v." (IFCLABEL)
  Green Building Properties | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    NOx Emissions (air free, 0% O2) ppm = "" (IFCTEXT)
    NOx Emissions mg/kWh = "" (IFCTEXT)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Diameter = 730. (IFCLENGTHMEASURE) [MILLI METRE]
    Flue Diameter - concentric system = "100/150 mm/mm" (IFCTEXT)
    Flue Diameter - parallel system = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    Flue Diameter - water heater = "100/150 mm/mm" (IFCTEXT)
    Height = 1655. (IFCLENGTHMEASURE) [MILLI METRE]
    Height Air Inlet = 385. (IFCLENGTHMEASURE) [MILLI METRE]
    Height Cold water Intlet = 400. (IFCLENGTHMEASURE) [MILLI METRE]
    Height Flue Outlet = 385. (IFCLENGTHMEASURE) [MILLI METRE]
    Height Gas Connection = 160. (IFCLENGTHMEASURE) [MILLI METRE]
    Height Warm Water Outlet = 1655. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Mechanical - Flow | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Draw-off Capacity @ ΔT = 28°C after 120 min. = 116.538400180912 (IFCREAL)
    Draw-off Capacity @ ΔT = 28°C after 30 min. = 38.8461333936374 (IFCREAL)
    Draw-off Capacity @ ΔT = 28°C after 60 min. = 67.0978667708283 (IFCREAL)
    Draw-off Capacity @ ΔT = 28°C after 90 min. = 91.8181334758703 (IFCREAL)
    Draw-off Capacity @ ΔT = 44°C after 120 min. = 74.160800115126 (IFCREAL)
    Draw-off Capacity @ ΔT = 44°C after 30 min. = 23.6608267033974 (IFCREAL)
    Draw-off Capacity @ ΔT = 44°C after 60 min. = 42.3776000657863 (IFCREAL)
    Draw-off Capacity @ ΔT = 44°C after 90 min. = 56.5034667543817 (IFCREAL)
    Draw-off Capacity @ ΔT = 50°C after 120 min. = 67.0978667708283 (IFCREAL)
    Draw-off Capacity @ ΔT = 50°C after 30 min. = 20.4825066984634 (IFCREAL)
    Draw-off Capacity @ ΔT = 50°C after 60 min. = 34.9615200542737 (IFCREAL)
    Draw-off Capacity @ ΔT = 50°C after 90 min. = 49.440533410084 (IFCREAL)
    Draw-off Capacity @ ΔT = 55°C after 120 min. = 60.0349334265306 (IFCREAL)
    Draw-off Capacity @ ΔT = 55°C after 30 min. = 18.3636266951741 (IFCREAL)
    Draw-off Capacity @ ΔT = 55°C after 60 min. = 31.4300533821248 (IFCREAL)
    Draw-off Capacity @ ΔT = 55°C after 90 min. = 45.9090667379352 (IFCREAL)
    Draw-off Capacity @ ΔT = 70°C after 120 min. = 45.9090667379352 (IFCREAL)
    Draw-off Capacity @ ΔT = 70°C after 30 min. = 13.4195733541657 (IFCREAL)
    Draw-off Capacity @ ΔT = 70°C after 60 min. = 23.6608267033974 (IFCREAL)
    Draw-off Capacity @ ΔT = 70°C after 90 min. = 34.2552267198439 (IFCREAL)
    Heating Up Time @ ΔT = 28°C = "8" (IFCTEXT)
    Heating Up Time @ ΔT = 44°C = "12" (IFCTEXT)
    Heating Up Time @ ΔT = 50°C = "14" (IFCTEXT)
    Heating Up Time @ ΔT = 55°C = "15" (IFCTEXT)
    Heating Up Time @ ΔT = 70°C = "19" (IFCTEXT)
    Recovery Rate @ ΔT = 28°C = 1.5 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Recovery Rate @ ΔT = 44°C = 0.94 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Recovery Rate @ ΔT = 50°C = 0.83 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Recovery Rate @ ΔT = 55°C = 0.75 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Recovery Rate @ ΔT = 70°C = 0.59 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
  General | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    1e Maintenance (check-up) = "3 months after installation" (IFCTEXT)
    2nd Maintenance (general maintenance) = "12 months after installation" (IFCTEXT)
    Maintenance Interval = "12" (IFCTEXT)
    Packaging Height = 1750. (IFCLENGTHMEASURE) [MILLI METRE]
    Packaging Length = 870. (IFCLENGTHMEASURE) [MILLI METRE]
    Packaging Width = 780. (IFCLENGTHMEASURE) [MILLI METRE]
    Transport Weight = 100. (IFCREAL)
    Type of Packaging = "Plastic Shrink Wrap, Cardboard and Wood" (IFCTEXT)
    Warranty on parts = "12 months" (IFCTEXT)
    Warranty on tank = "36 months" (IFCTEXT)
  Plumbing | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Cold Water Connection R = 0.0833333333333333 (IFCREAL)
    Condens Discharge Connection = 1. (IFCLENGTHMEASURE) [MILLI METRE]
    Drain Valve Connection Rp = 0.0625 (IFCREAL)
    Gas Connection R = 0.0416666666666667 (IFCREAL)
    Hot / Warm Water Connection R = 0.0833333333333333 (IFCREAL)
    T&P Connection Rp = 0.0833333333333333 (IFCREAL)
  Model Properties | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Co2 Emissions (tol. +/- 1.0) vol% = "10.4" (IFCTEXT)
    Default Setpoint = 338.15 (IFCREAL)
    Empty Weight = 82. (IFCREAL)
    Gas Flow Rate - Mass kg/h = 3.5 (IFCREAL)
    Gas Flow Rate - Volume ltr/hr = 0. (IFCREAL)
    Insulation Thickness = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Max. Flue Gas Outlet Temperature = 338.15 (IFCREAL)
    Max. Operating Pressure = 243840. (IFCREAL)
    Max. Setpoint = 358.15 (IFCREAL)
    Min. Setpoint = 283.15 (IFCREAL)
    Noice-level dB (A) = "58" (IFCTEXT)
    Nominal Heat Input (Gross) = 513438.526877054 (IFCREAL)
    Nominal Heat Input (Net) = 484375.968751938 (IFCREAL)
    Nominal Output = 526355.219377105 (IFCREAL)
    Operating Weight = 271. (IFCREAL)
    Stand-by Loss - daily (24h) = 0. (IFCREAL)
    Stand-by Loss = 0. (IFCREAL)
    Storage Capacity = 6.67447201036134 (IFCREAL)
    Supply Pressure = 1127.76 (IFCREAL)
  Electrical | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    (Additional Control) Frequency = 0. (IFCREAL)
    (Additional Control) Phase = 1 (IFCINTEGER)
    (Additional Control) Power Consumption (nominal) = 0. (IFCREAL)
    (Additional Control) Voltage = 0. (IFCREAL)
    Frequency = 50. (IFCREAL)
    Phase = 1 (IFCINTEGER)
    Power Consumption (nominal) = 3229.17312501292 (IFCREAL)
    Voltage = 2475.69939584324 (IFCREAL)
  Energy Analysis | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Energy Efficiency Rating (Hi, acc NEN-EN 89-1999) = 106. (IFCREAL)
    Energy Efficiency Rating (Hs, acc NEN-EN 89-1999) = 95. (IFCREAL)
    Seasonal Energy Efficiency Rating = 91. (IFCREAL)