IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
File name: "0001"
Time stamp: "2017-02-16T16:24:37"
Preprocessor: "The EXPRESS Data Manager Version 5.01.0100.02.64mod : 6 Jun 2012"
Originating system: "20140709_2115(x64) - Exporter 3.13.0.0 - Alternate UI 2.13.0.1"
Application: "Autodesk Revit 2014 (ENU)" version "2014" identifier "Revit" by Organization "Autodesk Revit 2014 (ENU)"

People and organizations
  Person "MMT" of Organization (no name given)
  Owner history of Person "MMT" of Organization (no name given) | application "Autodesk Revit 2014 (ENU)" version "2014" identifier "Revit" by Organization "Autodesk Revit 2014 (ENU)" | change NOCHANGE | created 1487258295 (2017-02-16T15:18:15Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  PRESSUREUNIT: PASCAL

Spatial structure
IFCPROJECT "0001" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 30.344238″ | longitude -71° 3′ 35.194702″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "<Default>"
      IFCBUILDINGSTOREY "BFC" | long name "BFC" | elevation 0.
        contains 8 elements
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Condensing-Storage-Water-Heater-Gas_AO_Smith-BFC_30_N" | object type "Condensing-Storage-Water-Heater-Gas_AO_Smith-BFC_30_N" | names: "Condensing-Storage-Water-Heater-Gas_AO_Smith-BFC_30_N:Condensing-Storage-Water-Heater-Gas_AO_Smith-BFC_30_N:804719" | material: materials ("XX_AO Smith - RAL 1036", "RAL 9011", "XX_AO Smith - RAL 9011", "RAL 1036", "Workspace 3D") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Constraints, Identity Data, Mechanical, Other
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Condensation drainage (internal)" | object type "Condensation drainage (internal)" | names: "07_Condensation drainage (internal):Condensation drainage (internal):804720" | material: "XX_AO Smith - RAL 9005" | property sets: Pset_BuildingElementProxyCommon, Constraints, Identity Data, Phasing
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "09_BCF 30-50-60 - Chimney Pipe" | object type "09_BCF 30-50-60 - Chimney Pipe" | names: "09_BCF 30-50-60 - Chimney Pipe:09_BCF 30-50-60 - Chimney Pipe:804721" | material: "Aluminium" | property sets: Pset_BuildingElementProxyCommon, Constraints, Identity Data, Phasing
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "01_Boiler ø705mm" | object type "01_Boiler ø705mm" | names: "01_Boiler ø705mm:01_Boiler ø705mm:804722" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Constraints, Identity Data, Phasing
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "02_Water control (external)" | object type "02_Water control (external)" | names: "02_Water control (external):02_Water control (external):804723" | material: "RAL 1036" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Constraints, Identity Data, Phasing
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "04_Tank drain valve (external)" | object type "04_Tank drain valve (external)" | names: "04_Tank drain valve (external):04_Tank drain valve (external):804725" | material: materials ("XX_AO Smith - RAL 1036", "XX_AO Smith - Aluminium") | property sets: Pset_BuildingElementProxyCommon, Constraints, Identity Data, Phasing
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Top ø705mm" | object type "Top ø705mm" | names: "08_Top Boiler ø705mm.rfa:Top ø705mm:804726" | material: materials ("Plastic, Opaque Black", "XX_AO Smith - Sticker BCF", "XX_AO Smith - RAL 9005") | property sets: Pset_BuildingElementProxyCommon, Constraints, Identity Data, Phasing
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "06_Cleaning and inspection opening" | object type "06_Cleaning and inspection opening" | names: "06_Cleaning and inspection opening:06_Cleaning and inspection opening:804727" | material: "RAL 9011" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Constraints, Identity Data, Phasing

Types
  IFCBUILDINGELEMENTPROXYTYPE "Condensing-Storage-Water-Heater-Gas_AO_Smith-BFC_30_N" | 1 occurrence | material: materials ("XX_AO Smith - RAL 1036", "RAL 9011", "XX_AO Smith - RAL 9011", "RAL 1036", "Workspace 3D") | property sets: Dimensions, Electrical, Energy Analysis, General, Green Building Properties, Identity Data
  IFCBUILDINGELEMENTPROXYTYPE "Condensation drainage (internal)" | 1 occurrence | material: "XX_AO Smith - RAL 9005" | property sets: Identity Data
  IFCBUILDINGELEMENTPROXYTYPE "09_BCF 30-50-60 - Chimney Pipe" | 1 occurrence | material: "Aluminium" | property sets: Identity Data
  IFCBUILDINGELEMENTPROXYTYPE "01_Boiler ø705mm" | 1 occurrence | property sets: Dimensions, Identity Data
  IFCBUILDINGELEMENTPROXYTYPE "02_Water control (external)" | 1 occurrence | material: "RAL 1036" | property sets: Identity Data
  IFCBUILDINGELEMENTPROXYTYPE "04_Tank drain valve (external)" | 1 occurrence | material: materials ("XX_AO Smith - RAL 1036", "XX_AO Smith - Aluminium") | property sets: Identity Data
  IFCBUILDINGELEMENTPROXYTYPE "Top ø705mm" | 1 occurrence | material: materials ("Plastic, Opaque Black", "XX_AO Smith - Sticker BCF", "XX_AO Smith - RAL 9005") | property sets: Identity Data
  IFCBUILDINGELEMENTPROXYTYPE "06_Cleaning and inspection opening" | 1 occurrence | material: "RAL 9011" | property sets: Identity Data

Property sets
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Host = "Level : BFC" (IFCTEXT)
    Level = "Level: BFC" (IFCLABEL)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Host = "Level : BFC" (IFCTEXT)
    Level = "Level: BFC" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 290. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Host = "Level : BFC" (IFCTEXT)
    Level = "Level: BFC" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 226.783037026766 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Host = "Level : BFC" (IFCTEXT)
    Level = "Level: BFC" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Host = "Level : BFC" (IFCTEXT)
    Level = "Level: BFC" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 160. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Host = "Level : BFC" (IFCTEXT)
    Level = "Level: BFC" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = -9.2932599030856 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Host = "Level : BFC" (IFCTEXT)
    Level = "Level: BFC" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 1566. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints: 2 more contents on 2 objects not shown
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Condensing-Storage-Water-Heater-Gas_AO_Smith-BFC_30_N" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Condensation drainage (internal)" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "09_BCF 30-50-60 - Chimney Pipe" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "01_Boiler ø705mm" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "02_Water control (external)" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "04_Tank drain valve (external)" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Top ø705mm" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "06_Cleaning and inspection opening" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    Manufacturer = "A.O. Smith" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Manufacturer = "A.O. Smith Water Products Company b.v." (IFCLABEL)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Mark = "166" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Mark = "167" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Mark = "168" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Mark = "169" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Mark = "170" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Mark = "172" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Mark = "173" (IFCTEXT)
  Identity Data: 7 more contents on 2 objects not shown
  Mechanical | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    System Classification = "Domestic Cold Water,Other,Domestic Hot Water,Other,Domestic Cold Water,Power" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 1 type object
    APS Pressure < = 115. (IFCPRESSUREMEASURE) [PASCAL]
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "0001" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Workspace = TRUE (IFCBOOLEAN)
  Phasing | properties | on 8 objects (8 IFCBUILDINGELEMENTPROXY)
    Phase Created = "Phase 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    Diameter = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    Flue Diameter - concentric system = "100/150 mm/mm" (IFCTEXT)
    Flue Diameter - parallel system = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    Flue Diameter - water heater = "100/150 mm/mm" (IFCTEXT)
    Height = 1910. (IFCLENGTHMEASURE) [MILLI METRE]
    Height Air Inlet = 1905. (IFCLENGTHMEASURE) [MILLI METRE]
    Height Cold water Intlet = 160. (IFCLENGTHMEASURE) [MILLI METRE]
    Height Flue Outlet = 1905. (IFCLENGTHMEASURE) [MILLI METRE]
    Height Gas Connection = 1815. (IFCLENGTHMEASURE) [MILLI METRE]
    Height Warm Water Outlet = 1910. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    A = 1910. (IFCLENGTHMEASURE) [MILLI METRE]
    K = 1566. (IFCLENGTHMEASURE) [MILLI METRE]
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Electrical | properties | on 1 type object
    (Additional Control) Frequency = 0. (IFCFREQUENCYMEASURE) [HERTZ]
    (Additional Control) Phase = 1 (IFCINTEGER)
    (Additional Control) Power Consumption (nominal) = 0. (IFCPOWERMEASURE) [WATT]
    (Additional Control) Voltage = 0. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    Frequency = 50. (IFCFREQUENCYMEASURE) [HERTZ]
    Phase = 1 (IFCINTEGER)
    Power Consumption (nominal) = 45. (IFCPOWERMEASURE) [WATT]
    Voltage = 230. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
  Energy Analysis | properties | on 1 type object
    Energy Efficiency Rating (Hi, acc NEN-EN 89-1999) = 109. (IFCREAL)
    Energy Efficiency Rating (Hs, acc NEN-EN 89-1999) = 98. (IFCREAL)
    Seasonal Energy Efficiency Rating = 98. (IFCREAL)
  General | properties | on 1 type object
    1e Maintenance (check-up) = "3 maanden na installatie" (IFCTEXT)
    2nd Maintenance (general maintenance) = "12 maanden na installatie" (IFCTEXT)
    Maintenance Interval = "12 maanden" (IFCTEXT)
    Packaging Height = 2080. (IFCLENGTHMEASURE) [MILLI METRE]
    Packaging Length = 950. (IFCLENGTHMEASURE) [MILLI METRE]
    Packaging Width = 790. (IFCLENGTHMEASURE) [MILLI METRE]
    Transport Weight = 235. (IFCREAL)
    Type of Packaging = "Plastic Krimpverpakking, Karton en Hout" (IFCTEXT)
    Warranty on parts = "12 maanden" (IFCTEXT)
    Warranty on tank = "36 maanden" (IFCTEXT)
  Green Building Properties | properties | on 1 type object
    NOx Emissions (air free, 0% O2) ppm = "18" (IFCTEXT)
    NOx Emissions mg/kWh = "32" (IFCTEXT)
  Mechanical - Flow | properties | on 1 type object
    Draw-off Capacity @ ΔT = 28°C after 120 min. = 2.5 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 28°C after 30 min. = 0.95 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 28°C after 60 min. = 1.5 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 28°C after 90 min. = 2. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 44°C after 120 min. = 1.5 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 44°C after 30 min. = 0.55 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 44°C after 60 min. = 0.87 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 44°C after 90 min. = 1.2 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 50°C after 120 min. = 1.3 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 50°C after 30 min. = 0.45 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 50°C after 60 min. = 0.73 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 50°C after 90 min. = 1.1 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 55°C after 120 min. = 1.2 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 55°C after 30 min. = 0.39 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 55°C after 60 min. = 0.65 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 55°C after 90 min. = 0.9 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 70°C after 120 min. = 0.84 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 70°C after 30 min. = 0.24 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 70°C after 60 min. = 0.44 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 70°C after 90 min. = 0.64 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Heating Up Time @ ΔT = 28°C = "22" (IFCTEXT)
    Heating Up Time @ ΔT = 44°C = "35" (IFCTEXT)
    Heating Up Time @ ΔT = 50°C = "39" (IFCTEXT)
    Heating Up Time @ ΔT = 55°C = "43" (IFCTEXT)
    Heating Up Time @ ΔT = 70°C = "55" (IFCTEXT)
    Recovery Rate @ ΔT = 28°C = 1.1 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Recovery Rate @ ΔT = 44°C = 0.64 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Recovery Rate @ ΔT = 50°C = 0.57 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Recovery Rate @ ΔT = 55°C = 0.52 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Recovery Rate @ ΔT = 70°C = 0.41 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
  Model Properties | properties | on 1 type object
    Co2 Emissions (tol. +/- 1.0) vol% = "9.0/9.1" (IFCTEXT)
    Default Setpoint = 65. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Empty Weight = 214. (IFCREAL)
    Gas Flow Rate - Mass kg/h = 0. (IFCREAL)
    Gas Flow Rate - Volume ltr/hr = "3.20/3.60" (IFCTEXT)
    Insulation Thickness = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Max. Flue Gas Outlet Temperature = 50. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Max. Operating Pressure = 800000. (IFCPRESSUREMEASURE) [PASCAL]
    Max. Setpoint = 80. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Min. Setpoint = 40. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Noice-level dB (A) = "45" (IFCTEXT)
    Nominal Heat Input (Gross) = "33300.0/33300.0" (IFCTEXT)
    Nominal Heat Input (Net) = "30000.0/30.000.0" (IFCTEXT)
    Nominal Output = "32700.0/32700.0" (IFCTEXT)
    Operating Weight = 582. (IFCREAL)
    Stand-by Loss - daily (24h) = 0. (IFCPOWERMEASURE) [WATT]
    Stand-by Loss = 0. (IFCPOWERMEASURE) [WATT]
    Storage Capacity = 0.368 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Supply Pressure = "2000/2500" (IFCTEXT)
  Plumbing | properties | on 1 type object
    Cold Water Connection R = 38.1 (IFCLENGTHMEASURE) [MILLI METRE]
    Condens Discharge Connection = 40. (IFCLENGTHMEASURE) [MILLI METRE]
    Drain Valve Connection Rp = 25.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Gas Connection R = 19.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Hot / Warm Water Connection R = 38.1 (IFCLENGTHMEASURE) [MILLI METRE]
    T&P Connection Rp = 25.4 (IFCLENGTHMEASURE) [MILLI METRE]