IFC building model
Schema: "IFC4"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "0001"
Time stamp: "2016-11-04T14:02:31"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20160512_0715(x64) - Exporter 15.7.0.0 - Default UI"
Application: "Autodesk Revit 2015 (ENU)" version "2015" identifier "Revit" by Organization "Autodesk Revit 2015 (ENU)"

People and organizations
  Person "michele.mollet@cadcompany.nl" of Organization (no name given)
  Owner history of Person "michele.mollet@cadcompany.nl" of Organization (no name given) | application "Autodesk Revit 2015 (ENU)" version "2015" identifier "Revit" by Organization "Autodesk Revit 2015 (ENU)" | change NOCHANGE | created 1478264548 (2016-11-04T13:02:28Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "0001" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 30.344238″ | longitude -71° 3′ 35.194702″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "<Default>"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 2 elements
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "IR-32-380 NL LP" | object type "IR-32-380 NL LP" | names: "Innovo NL_IR 32 380 NL LP:IR-32-380 NL LP:271355" | material: materials ("Rubber", "Aluminium", "RAL 9006", "RAL 9005", "display", "RAL 9011") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Constraints, Dimensions, Identity Data, Mechanical
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Workspace" | object type "Workspace" | names: "Innovo_workspace:Workspace:271358" | material: "Workspace 3D" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Constraints, Dimensions, Identity Data, Other

Types
  IFCBUILDINGELEMENTPROXYTYPE "IR-32-380 NL LP" | 1 occurrence | material: materials ("Rubber", "Aluminium", "RAL 9006", "RAL 9005", "display", "RAL 9011") | property sets: Constraints(Type), Dimensions(Type), Electrical(Type), Energy Analysis(Type), General(Type), Green Building Properties(Type)
  IFCBUILDINGELEMENTPROXYTYPE "Workspace" | 1 occurrence | material: "Workspace 3D" | property sets: Identity Data(Type), Other(Type)

Property sets
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other(Type) | properties | on 1 type object
    Category = "Mechanical Equipment" (IFCLABEL)
    Family Name = "Innovo NL_IR 32 380 NL LP" (IFCTEXT)
    Werkruimte Afstand Voor = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    Werkruimte Hoogte = 2745. (IFCLENGTHMEASURE) [MILLI METRE]
    Werkruimte Radius = 845. (IFCLENGTHMEASURE) [MILLI METRE]
  Other(Type) | properties | on 1 type object
    Category = "Mechanical Equipment" (IFCLABEL)
    Family Name = "Innovo_workspace" (IFCTEXT)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "0001" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Mechanical Equipment" (IFCLABEL)
    Family = "Innovo NL_IR 32 380 NL LP: IR-32-380 NL LP" (IFCLABEL)
    Family and Type = "Innovo NL_IR 32 380 NL LP: IR-32-380 NL LP" (IFCLABEL)
    Type = "Innovo NL_IR 32 380 NL LP: IR-32-380 NL LP" (IFCLABEL)
    Type Id = "Innovo NL_IR 32 380 NL LP: IR-32-380 NL LP" (IFCLABEL)
    Werkruimte = TRUE (IFCBOOLEAN)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Mechanical Equipment" (IFCLABEL)
    Family = "Innovo_workspace: Workspace" (IFCLABEL)
    Family and Type = "Innovo_workspace: Workspace" (IFCLABEL)
    Type = "Innovo_workspace: Workspace" (IFCLABEL)
    Type Id = "Innovo_workspace: Workspace" (IFCLABEL)
    Workspace = TRUE (IFCBOOLEAN)
    Workspace Distance Front = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    Workspace Height = 2745. (IFCLENGTHMEASURE) [MILLI METRE]
    Workspace Radius = 845. (IFCLENGTHMEASURE) [MILLI METRE]
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8mm Head" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "Level: 8mm Head" (IFCLABEL)
    Type Id = "Level: 8mm Head" (IFCLABEL)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Identity Data(Type) | properties | on 1 type object
    Assembly Code = "D3010" (IFCTEXT)
    Assembly Description = "Energy Supply" (IFCTEXT)
    BIM Content Developer = "CAD & Company" (IFCTEXT)
    Bestemming / Land = "Nederland" (IFCTEXT)
    CE-PIN = "0063CQ3037" (IFCTEXT)
    Created By = "http://www.cadcompany.nl/" (IFCTEXT)
    Description = "Condenserende Hoog Rendementsboiler" (IFCTEXT)
    Fabrikantnummer = "E 7110" (IFCTEXT)
    Gascategorie = "II2EK3B/P" (IFCTEXT)
    Installatie Typen = "B23/C13/C33/C43/C53/C63" (IFCTEXT)
    Manufacturer = "A.O. Smith Water Products Company b.v." (IFCTEXT)
    Model = "IR-32-380 NL LP" (IFCTEXT)
    OmniClass Number = "23.75.00.00" (IFCTEXT)
    OmniClass Title = "Climate Control (HVAC)" (IFCTEXT)
    Produkt Model Nummer (EAN-nummer) = "8717449283964" (IFCTEXT)
    Produkthandleiding Link = "" (IFCTEXT)
    Produktspecificaties Link = "" (IFCTEXT)
    Standaard Afgesteld op = "G30/G31" (IFCTEXT)
    Type Name = "IR-32-380 NL LP" (IFCTEXT)
    URL = "www.aosmith.nl" (IFCTEXT)
  Identity Data(Type) | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    BIM Content Developer = "CAD & Company" (IFCTEXT)
    Created By = "" (IFCTEXT)
    Description = "" (IFCTEXT)
    Manufacturer = "A.O. Smith Water Products Company b.v." (IFCTEXT)
    Model = "" (IFCTEXT)
    OmniClass Number = "23.75.00.00" (IFCTEXT)
    OmniClass Title = "Climate Control (HVAC)" (IFCTEXT)
    Type Name = "Workspace" (IFCTEXT)
    URL = "www.aosmith.nl" (IFCTEXT)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Mark = "1" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Mark = "2" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Constraints(Type) | properties | on 1 type object
    Kraan Hoogte 01 = 693. (IFCLENGTHMEASURE) [MILLI METRE]
    Kraan Hoogte 02 = 1518. (IFCLENGTHMEASURE) [MILLI METRE]
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "IR-32-380 NL LP" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Workspace" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Manufacturer = "A.O. Smith Water Products Company b.v." (IFCLABEL)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Host = "None" (IFCTEXT)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Host = "None" (IFCTEXT)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 3.81084377697952 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.704026111746583 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 11.420720887344 (IFCAREAMEASURE) [SQUARE_METRE]
    Center to Front = 552.825381227623 (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 6.99264905704617 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Mechanical | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    System Classification = "Domestic Hot Water,Other Air" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Phasing | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Phase Created = "Phase 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
    Reference = "Project Information" (IFCIDENTIFIER)
  Dimensions(Type) | properties | on 1 type object
    Breedte = 675. (IFCLENGTHMEASURE) [MILLI METRE]
    Diameter = 675. (IFCLENGTHMEASURE) [MILLI METRE]
    Diameter Schoorsteen - boiler = "80/125 mm/mm" (IFCTEXT)
    Diameter Schoorsteen - concentrisch systeem = "80/125 mm/mm" (IFCTEXT)
    Diameter Schoorsteen - parallel systeem = "2x80" (IFCTEXT)
    Hoogte = 1745. (IFCLENGTHMEASURE) [MILLI METRE]
    Hoogte Gas Aansluiting = 905. (IFCLENGTHMEASURE) [MILLI METRE]
    Hoogte Koud Water Inlaat = 170. (IFCLENGTHMEASURE) [MILLI METRE]
    Hoogte Lucht Inlaat = 1350. (IFCLENGTHMEASURE) [MILLI METRE]
    Hoogte Rookgasafvoer = 1350. (IFCLENGTHMEASURE) [MILLI METRE]
    Hoogte Warm Water Uitlaat = 1745. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 780. (IFCLENGTHMEASURE) [MILLI METRE]
  Electrical(Type) | properties | on 1 type object
    Elektrisch Vermogen (nominaal) = 85. (IFCPOWERMEASURE) [WATT]
    Elektrisch Vermogen (piek) = 105. (IFCPOWERMEASURE) [WATT]
    Fase = 1 (IFCINTEGER)
    Frequentie = 50. (IFCFREQUENCYMEASURE) [HERTZ]
    Voltage = 230. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
  Energy Analysis(Type) | properties | on 1 type object
    Ander capaciteitsprofiel = "3XL" (IFCTEXT)
    Capaciteitsprofiel = "XXL" (IFCTEXT)
    Energie-efficiëntie voor waterverwarming (1) = "90%" (IFCTEXT)
    Energie-efficiëntie voor waterverwarming (2) = "92%" (IFCTEXT)
    Energie-efficiëntieklasse voor waterverwarming (1) = "A" (IFCTEXT)
    Energie-efficiëntieklasse voor waterverwarming (2) = "-" (IFCTEXT)
    Geluidsniveau binnen = "58 dB" (IFCTEXT)
    Handelsmerk = "A.O. Smith" (IFCTEXT)
    Jaarlijks brandstofverbruik (1) = "21 GJ GCV" (IFCTEXT)
    Jaarlijks brandstofverbruik (2) = "40 GJ GCV" (IFCTEXT)
    Jaarlijks elektriciteitsverbruik (1) = "45 kWh" (IFCTEXT)
    Jaarlijks elektriciteitsverbruik (2) = "92 kWh" (IFCTEXT)
    Rendement (Hi, vlgs. NEN-EN 89 - 1999) = 108. (IFCREAL)
    Rendement (Hs, vlgs. NEN-EN 89 - 1999) = 97. (IFCREAL)
    Seizoens Rendement (Hs) = 97. (IFCREAL)
    Setpoint thermostaat = 65. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Slimme controlefunctie = FALSE (IFCBOOLEAN)
    Type aanduiding = "IR-32-380" (IFCTEXT)
    Uitsluitend werkend in daluren = FALSE (IFCBOOLEAN)
    Voorzorgsmaatregelen tijdens montage, installatie of onderhoud = "zie Gebruikers, Installatie, Service en Onderhouds handleiding" (IFCTEXT)
  General(Type) | properties | on 1 type object
    1e Onderhoud (check-up) = "3 maanden na installatie" (IFCTEXT)
    2e Onderhoud (algeheel onderhoud) = "12 maanden na installatie" (IFCTEXT)
    Garrantie op Onderdelen = "12 maanden" (IFCTEXT)
    Garrantie op Tank = "36 maanden" (IFCTEXT)
    Onderhoudsinterval = "12 maanden" (IFCTEXT)
    Soort Verpakking = "Karton en Hout" (IFCTEXT)
    Transportgewicht = 172. (IFCREAL)
    Verpakkingsbreedte = 786. (IFCLENGTHMEASURE) [MILLI METRE]
    Verpakkingshoogte = 1895. (IFCLENGTHMEASURE) [MILLI METRE]
    Verpakkingslengte = 946. (IFCLENGTHMEASURE) [MILLI METRE]
  Green Building Properties(Type) | properties | on 1 type object
    NOx-uitstoot (lucht vrij, 0% O2) ppm = "63.0/23.0" (IFCTEXT)
    NOx-uitstoot mg/kWh = "103.0/37.0" (IFCTEXT)
  Mechanical - Flow(Type) | properties | on 1 type object
    Opwarmtijd bij ΔT = 28°C = "20" (IFCTEXT)
    Opwarmtijd bij ΔT = 44°C = "31" (IFCTEXT)
    Opwarmtijd bij ΔT = 50°C = "36" (IFCTEXT)
    Opwarmtijd bij ΔT = 55°C = "39" (IFCTEXT)
    Opwarmtijd bij ΔT = 70°C = "50" (IFCTEXT)
    Tapcapaciteit Continu bij ΔT = 28°C = 33.902080052629 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Tapcapaciteit Continu bij ΔT = 44°C = 21.1888000328932 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Tapcapaciteit Continu bij ΔT = 50°C = 18.7167733623889 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Tapcapaciteit Continu bij ΔT = 55°C = 16.9510400263145 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Tapcapaciteit Continu bij ΔT = 70°C = 13.4195733541657 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Tapcapaciteit bij ΔT = 28°C na 120 min. = 2.8 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Tapcapaciteit bij ΔT = 28°C na 30 min. = 1.3 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Tapcapaciteit bij ΔT = 28°C na 60 min. = 1.8 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Tapcapaciteit bij ΔT = 28°C na 90 min. = 2.3 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Tapcapaciteit bij ΔT = 44°C na 120 min. = 1.4 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Tapcapaciteit bij ΔT = 44°C na 30 min. = 1.8 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Tapcapaciteit bij ΔT = 44°C na 60 min. = 0.79 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Tapcapaciteit bij ΔT = 44°C na 90 min. = 1.1 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Tapcapaciteit bij ΔT = 50°C na 120 min. = 1.5 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Tapcapaciteit bij ΔT = 50°C na 30 min. = 0.68 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Tapcapaciteit bij ΔT = 50°C na 60 min. = 0.95 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Tapcapaciteit bij ΔT = 50°C na 90 min. = 1.3 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Tapcapaciteit bij ΔT = 55°C na 120 min. = 1.4 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Tapcapaciteit bij ΔT = 55°C na 30 min. = 0.61 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Tapcapaciteit bij ΔT = 55°C na 60 min. = 0.86 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Tapcapaciteit bij ΔT = 55°C na 90 min. = 1.1 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Tapcapaciteit bij ΔT = 70°C na 120 min. = 1.1 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Tapcapaciteit bij ΔT = 70°C na 30 min. = 0.46 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Tapcapaciteit bij ΔT = 70°C na 60 min. = 0.65 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Tapcapaciteit bij ΔT = 70°C na 90 min. = 0.84 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Mechanical(Type) | properties | on 1 type object
    Uitschakeldruk LDS < = 210. (IFCPRESSUREMEASURE) [PASCAL]
  Model Properties(Type) | properties | on 1 type object
    CO2-uitstoot (tol. +/- 1.0) vol% = "11.8/10.0" (IFCTEXT)
    Gas Voordruk = 5000. (IFCPRESSUREMEASURE) [PASCAL]
    Gasverbruik - Massa kg/h = "2.60/2.30" (IFCTEXT)
    Gasverbruik - Volume ltr/hr = "n.v.t." (IFCTEXT)
    Geluidsniveau dB (A) = "<45" (IFCTEXT)
    Inhoud = 0.38 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Isolatiedikte = 44. (IFCLENGTHMEASURE) [MILLI METRE]
    Ledig Gewicht = 155. (IFCREAL)
    Max. Rookgastemperatuur = 65. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Max. Stand Regelthermostaat = 85. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Max. Werkdruk = 800000. (IFCPRESSUREMEASURE) [PASCAL]
    Min. Stand Regelthermostaat = 40. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Nominaal Vermogen = "34800.0/30700.0" (IFCTEXT)
    Nominale Belasting (Bovenwaarde) = "35800.0/31500.0" (IFCTEXT)
    Nominale Belasting (Onderwaarde) = "33000.0/29000.0" (IFCTEXT)
    Stand Regelthermostaat = 65. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Stilstandsverlies - dagelijks (24u) = 0. (IFCPOWERMEASURE) [WATT]
    Stilstandsverlies = 0. (IFCPOWERMEASURE) [WATT]
    Totaal Gewicht = 552. (IFCREAL)
  Plumbing(Type) | properties | on 1 type object
    Aansluiting Aftapkraan = 19.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Aansluiting Condensafvoer = 40. (IFCLENGTHMEASURE) [MILLI METRE]
    Aansluiting Koud Water = 19.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Aansluiting T&P = 25.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Aansluiting Warm Water = 25.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Gas Aansluiting = 381. (IFCLENGTHMEASURE) [MILLI METRE]