IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
File name: "0001"
Time stamp: "2015-05-07T11:48:32"
Preprocessor: "The EXPRESS Data Manager Version 5.01.0100.02.64mod : 6 Jun 2012"
Originating system: "20130308_1515(x64) - Exporter 2014.0.2013.0308 - Default UI"
Application: "Autodesk Revit 2014 (ENU)" version "2014" identifier "Revit" by Organization "Autodesk Revit 2014 (ENU)"

People and organizations
  Person "BTN" of Organization (no name given)
  Owner history of Person "BTN" of Organization (no name given) | application "Autodesk Revit 2014 (ENU)" version "2014" identifier "Revit" by Organization "Autodesk Revit 2014 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: KELVIN
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  POWERUNIT: WATT

Spatial structure
IFCPROJECT "0001" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 30.344238″ | longitude -71° 3′ 35.194702″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "<Default>"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 9 elements
          1 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "Condensing-Solar-Storage-Water-Heater-Gas_AO_Smith-SGS_30_PB" | object type "Condensing-Solar-Storage-Water-Heater-Gas_AO_Smith-SGS_30_PB" | names: "Condensing-Solar-Storage-Water-Heater-Gas_AO_Smith-SGS_30_PB:Condensing-Solar-Storage-Water-Heater-Gas_AO_Smith-SGS_30_PB:572907" | material: materials ("XX_AO Smith - RAL 1036", "RAL 9011", "XX_AO Smith - RAL 9011", "Workspace 3D") | property sets: Other, Phasing, Constraints, Identity Data, Electrical - Loads, Mechanical
          1 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "01_Boiler ø705mm" | object type "01_Boiler ø705mm" | names: "01_Boiler ø705mm:01_Boiler ø705mm:572909" | property sets: Constraints, Phasing, Identity Data, Pset_ManufacturerTypeInformation, Dimensions
          1 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "Water control (external)" | object type "Water control (external)" | names: "02_Water control (external):Water control (external):572910" | material: materials ("Rubber", "RAL 1036") | property sets: Constraints, Identity Data, Phasing, Pset_ManufacturerTypeInformation
          1 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "04_Tank drain valve (external)" | object type "04_Tank drain valve (external)" | names: "04_Tank drain valve (external):04_Tank drain valve (external):572912" | material: materials ("XX_AO Smith - RAL 1036", "XX_AO Smith - Aluminium", "XX_AO Smith - RAL 3000") | property sets: Identity Data, Constraints, Phasing
          1 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "Cleaning and inspection opening" | object type "Cleaning and inspection opening" | names: "06_Cleaning and inspection opening:Cleaning and inspection opening:572914" | material: "RAL 9011" | property sets: Constraints, Phasing, Identity Data, Pset_ManufacturerTypeInformation
          1 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "10_Temperature sensor" | object type "10_Temperature sensor" | names: "10_Temperature sensor:10_Temperature sensor:572915" | material: "RAL 9011" | property sets: Identity Data, Phasing, Constraints
          1 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "07. Condensation drainage (internal)" | object type "07. Condensation drainage (internal)" | names: "07. Condensation drainage (internal):07. Condensation drainage (internal):572917" | material: "RAL 9011" | property sets: Identity Data, Phasing, Constraints, Pset_ManufacturerTypeInformation
          1 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "09_BCF 30-50-60 - Chimney Pipe" | object type "09_BCF 30-50-60 - Chimney Pipe" | names: "09_BCF 30-50-60 - Chimney Pipe:09_BCF 30-50-60 - Chimney Pipe:572918" | material: "Aluminium" | property sets: Identity Data, Phasing, Constraints
          1 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "13_Base" | object type "13_Base" | names: "13_Base:13_Base:572919" | material: "RAL 9011" | property sets: Identity Data, Constraints, Phasing

Types
  IFCBOILERTYPE "Condensing-Solar-Storage-Water-Heater-Gas_AO_Smith-SGS_30_PB" | element type "Condensing-Solar-Storage-Water-Heater-Gas_AO_Smith-SGS_30_PB" | 1 occurrence | material: materials ("XX_AO Smith - RAL 1036", "RAL 9011", "XX_AO Smith - RAL 9011", "Workspace 3D")
  IFCBOILERTYPE "01_Boiler ø705mm" | element type "01_Boiler ø705mm" | 1 occurrence
  IFCBOILERTYPE "Water control (external)" | element type "Water control (external)" | 1 occurrence | material: materials ("Rubber", "RAL 1036")
  IFCBOILERTYPE "04_Tank drain valve (external)" | element type "04_Tank drain valve (external)" | 1 occurrence | material: materials ("XX_AO Smith - RAL 1036", "XX_AO Smith - Aluminium", "XX_AO Smith - RAL 3000")
  IFCBOILERTYPE "Cleaning and inspection opening" | element type "Cleaning and inspection opening" | 1 occurrence | material: "RAL 9011"
  IFCBOILERTYPE "10_Temperature sensor" | element type "10_Temperature sensor" | 1 occurrence | material: "RAL 9011"
  IFCBOILERTYPE "07. Condensation drainage (internal)" | element type "07. Condensation drainage (internal)" | 1 occurrence | material: "RAL 9011"
  IFCBOILERTYPE "09_BCF 30-50-60 - Chimney Pipe" | element type "09_BCF 30-50-60 - Chimney Pipe" | 1 occurrence | material: "Aluminium"
  IFCBOILERTYPE "13_Base" | element type "13_Base" | 1 occurrence | material: "RAL 9011"

Property sets
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 100. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 255.004625000003 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 85.3752966495128 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 280. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 95.0046250000028 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 116.613466520526 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints: 3 more contents on 3 objects not shown
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Other | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Workspace = TRUE (IFCBOOLEAN)
  Other | properties | on 1 object (1 IFCBUILDING)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "0001" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Phasing | properties | on 9 objects (9 IFCENERGYCONVERSIONDEVICE)
    Phase Created = "New Construction" (IFCLABEL)
  Identity Data | properties | on 4 objects (4 IFCENERGYCONVERSIONDEVICE)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Mark = "1" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Mark = "2" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Mark = "3" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Manufacturer = "A.O. Smith" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    Type Comments = "Condensation drainage (interna" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Mark = "5" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Mark = "7" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Manufacturer = "A.O. Smith" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    Type Comments = "Cleaning and inspection opening" (IFCTEXT)
  Identity Data: 9 more contents on 9 objects not shown
  Electrical - Loads | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Circuit Number = "" (IFCTEXT)
    Panel = "" (IFCTEXT)
  Mechanical | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    System Classification = "Domestic Cold Water,Other,Domestic Hot Water,Other,Domestic Cold Water,Power" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    APS Pressure < = 35.052 (IFCREAL)
  Pset_ManufacturerTypeInformation | properties | on 4 objects (4 IFCENERGYCONVERSIONDEVICE)
    Manufacturer = "A.O. Smith" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Manufacturer = "A.O. Smith Water Products Company b.v." (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Diameter = 705. (IFCLENGTHMEASURE) [MILLI METRE]
    Flue Diameter - concentric system = "100/150 mm/mm" (IFCTEXT)
    Flue Diameter - parallel system = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    Flue Diameter - water heater = "100/150 mm/mm" (IFCTEXT)
    Height = 2005. (IFCLENGTHMEASURE) [MILLI METRE]
    Height Air Inlet = 2000. (IFCLENGTHMEASURE) [MILLI METRE]
    Height Cold water Intlet = 255. (IFCLENGTHMEASURE) [MILLI METRE]
    Height Flue Outlet = 2000. (IFCLENGTHMEASURE) [MILLI METRE]
    Height Gas Connection = 1810. (IFCLENGTHMEASURE) [MILLI METRE]
    Height Warm Water Outlet = 2005. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 925. (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 850. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    A = 1810. (IFCLENGTHMEASURE) [MILLI METRE]
    K = 1466. (IFCLENGTHMEASURE) [MILLI METRE]
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Mechanical - Flow | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Draw-off Capacity @ ΔT = 28°C after 120 min. = 84.7552001315726 (IFCREAL)
    Draw-off Capacity @ ΔT = 28°C after 30 min. = 28.9580267116206 (IFCREAL)
    Draw-off Capacity @ ΔT = 28°C after 60 min. = 49.440533410084 (IFCREAL)
    Draw-off Capacity @ ΔT = 28°C after 90 min. = 67.0978667708283 (IFCREAL)
    Draw-off Capacity @ ΔT = 44°C after 120 min. = 49.440533410084 (IFCREAL)
    Draw-off Capacity @ ΔT = 44°C after 30 min. = 15.538453357455 (IFCREAL)
    Draw-off Capacity @ ΔT = 44°C after 60 min. = 26.8391467083313 (IFCREAL)
    Draw-off Capacity @ ΔT = 44°C after 90 min. = 38.8461333936374 (IFCREAL)
    Draw-off Capacity @ ΔT = 50°C after 120 min. = 42.3776000657863 (IFCREAL)
    Draw-off Capacity @ ΔT = 50°C after 30 min. = 12.360133352521 (IFCREAL)
    Draw-off Capacity @ ΔT = 50°C after 60 min. = 22.6013867017527 (IFCREAL)
    Draw-off Capacity @ ΔT = 50°C after 90 min. = 32.4894933837695 (IFCREAL)
    Draw-off Capacity @ ΔT = 55°C after 120 min. = 38.8461333936374 (IFCREAL)
    Draw-off Capacity @ ΔT = 55°C after 30 min. = 10.2412533492317 (IFCREAL)
    Draw-off Capacity @ ΔT = 55°C after 60 min. = 19.4230666968187 (IFCREAL)
    Draw-off Capacity @ ΔT = 55°C after 90 min. = 28.2517333771909 (IFCREAL)
    Draw-off Capacity @ ΔT = 70°C after 120 min. = 0. (IFCREAL)
    Draw-off Capacity @ ΔT = 70°C after 30 min. = 0. (IFCREAL)
    Draw-off Capacity @ ΔT = 70°C after 60 min. = 0. (IFCREAL)
    Draw-off Capacity @ ΔT = 70°C after 90 min. = 0. (IFCREAL)
    Heating Up Time @ ΔT = 28°C = "22" (IFCTEXT)
    Heating Up Time @ ΔT = 44°C = "35" (IFCTEXT)
    Heating Up Time @ ΔT = 50°C = "39" (IFCTEXT)
    Heating Up Time @ ΔT = 55°C = "43" (IFCTEXT)
    Heating Up Time @ ΔT = 70°C = "" (IFCTEXT)
    Recovery Rate @ ΔT = 28°C = 1.1 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Recovery Rate @ ΔT = 44°C = 0.64 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Recovery Rate @ ΔT = 50°C = 0.57 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Recovery Rate @ ΔT = 55°C = 0.52 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Recovery Rate @ ΔT = 70°C = 0. (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
  Electrical | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    (Additional Control) Frequency = 50. (IFCREAL)
    (Additional Control) Phase = 1 (IFCINTEGER)
    (Additional Control) Power Consumption (nominal) = 7534.73729169681 (IFCREAL)
    (Additional Control) Voltage = 2475.69939584324 (IFCREAL)
    Frequency = 50. (IFCREAL)
    Phase = 1 (IFCINTEGER)
    Power Consumption (nominal) = 484.375968751937 (IFCREAL)
    Voltage = 2475.69939584324 (IFCREAL)
  Plumbing | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Cold Water Connection R = 0.125 (IFCREAL)
    Condens Discharge Connection = 40. (IFCLENGTHMEASURE) [MILLI METRE]
    Drain Valve Connection Rp = 0.0833333333333333 (IFCREAL)
    Gas Connection R = 0.0625 (IFCREAL)
    Hot / Warm Water Connection R = 0.125 (IFCREAL)
    T&P Connection Rp = 0.0833333333333333 (IFCREAL)
  Model Properties | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Co2 Emissions (tol. +/- 1.0) vol% = "10,00" (IFCTEXT)
    Default Setpoint = 338.15 (IFCREAL)
    Empty Weight = 214. (IFCREAL)
    Gas Flow Rate - Mass kg/h = "2,30" (IFCTEXT)
    Gas Flow Rate - Volume ltr/hr = 0. (IFCREAL)
    Insulation Thickness = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Max. Flue Gas Outlet Temperature = 323.15 (IFCREAL)
    Max. Operating Pressure = 243840. (IFCREAL)
    Max. Setpoint = 353.15 (IFCREAL)
    Min. Setpoint = 313.15 (IFCREAL)
    Noice-level dB (A) = "45" (IFCTEXT)
    Nominal Heat Input (Gross) = "32600,0" (IFCTEXT)
    Nominal Heat Input (Net) = "30000,0" (IFCTEXT)
    Nominal Output = "32700,0" (IFCTEXT)
    Operating Weight = 582. (IFCREAL)
    Stand-by Loss - daily (24h) = 0. (IFCREAL)
    Stand-by Loss = 0. (IFCREAL)
    Storage Capacity = 12.9957973535078 (IFCREAL)
    Supply Pressure min/max = "3700" (IFCTEXT)
  General | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    1e Maintenance (check-up) = "3 maanden na installatie" (IFCTEXT)
    2nd Maintenance (general maintenance) = "12 maanden na installatie" (IFCTEXT)
    Maintenance Interval = "12 maanden" (IFCTEXT)
    Packaging Height = 2055. (IFCLENGTHMEASURE) [MILLI METRE]
    Packaging Length = 950. (IFCLENGTHMEASURE) [MILLI METRE]
    Packaging Width = 870. (IFCLENGTHMEASURE) [MILLI METRE]
    Transport Weight = 259. (IFCREAL)
    Type of Packaging = "Plastic Krimpverpakking, Karton en Hout" (IFCTEXT)
    Warranty on parts = "12 maanden" (IFCTEXT)
    Warranty on tank = "36 maanden" (IFCTEXT)
  Green Building Properties | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    NOx Emissions (air free, 0% O2) ppm = "41.0" (IFCTEXT)
    NOx Emissions mg/kWh = "74.0" (IFCTEXT)
  Energy Analysis | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Energy Efficiency Rating (Hi, acc NEN-EN 89-1999) = 109. (IFCREAL)
    Energy Efficiency Rating (Hs, acc NEN-EN 89-1999) = 98. (IFCREAL)
    Seasonal Energy Efficiency Rating = 98. (IFCREAL)