IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Condensing-Solar-Storage-Water-Heater-Gas_AO_Smith-SGS_80_G.ifc"
Time stamp: "2014-03-02T15:25:05"
Preprocessor: "Autodesk Revit 2013"
Originating system: "20130531_2115(x64)"
Application: "Autodesk Revit 2013" version "2013" identifier "Revit" by Organization "Autodesk Revit 2013"

People and organizations
  Person "TBR" of Organization (no name given)
  Owner history of Person "TBR" of Organization (no name given) | application "Autodesk Revit 2013" version "2013" identifier "Revit" by Organization "Autodesk Revit 2013" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: MILLI SQUARE_METRE
  VOLUMEUNIT: MILLI CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  TIMEUNIT: SECOND

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 30.344238″ | longitude -71° 3′ 35.194702″ | elevation above sea level -0.
    IFCBUILDING | postal address: "Enter address here", "<Default>"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 5 elements
          1 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "Condensing-Solar-Storage-Water-Heater-Gas_AO_Smith-SGS_80_G" | object type "Condensing-Solar-Storage-Water-Heater-Gas_AO_Smith-SGS_80_G" | names: "Condensing-Solar-Storage-Water-Heater-Gas_AO_Smith-SGS_80_G:Condensing-Solar-Storage-Water-Heater-Gas_AO_Smith-SGS_80_G:Condensing-Solar-Storage-Water-Heater-Gas_AO_Smith-SGS_80_G:193621" | material: materials ("RAL 1036", "Rubber", "Aluminium", "RAL 3000", "RAL 9011", "RAL 9005", "BCF Cyclone III - Sticker Membrane Control Panel", "Workspace 3D") | property sets: Mechanical, Identity Data, Constraints, Other, Phasing, Mechanical - Flow
          1 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "09.Boiler - ø850" | object type "09.Boiler - ø850" | names: "09.Boiler - ø850:09.Boiler - ø850:09.Boiler - ø850:193623" | material: "RAL 9006" | property sets: Identity Data, Constraints, Phasing, Dimensions
          1 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "12. Temperature sensor" | object type "12. Temperature sensor" | names: "12. Temperature sensor:12. Temperature sensor:12. Temperature sensor:193624" | material: "RAL 9011" | property sets: Phasing, Constraints, Identity Data
          1 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "11. BCF 80-100-120 - Chimney Pipe" | object type "11. BCF 80-100-120 - Chimney Pipe" | names: "11. BCF 80-100-120 - Chimney Pipe:11. BCF 80-100-120 - Chimney Pipe:11. BCF 80-100-120 - Chimney Pipe:193625" | material: "Aluminium" | property sets: Identity Data, Constraints, Phasing
          1 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "07. Condensation drainage (internal)" | object type "07. Condensation drainage (internal)" | names: "07. Condensation drainage (internal):07. Condensation drainage (internal):07. Condensation drainage (internal):193626" | material: "RAL 9011" | property sets: Identity Data, Phasing, Constraints

Types
  IFCBOILERTYPE "Condensing-Solar-Storage-Water-Heater-Gas_AO_Smith-SGS_80_G" | element type "Condensing-Solar-Storage-Water-Heater-Gas_AO_Smith-SGS_80_G" | 1 occurrence
  IFCBOILERTYPE "09.Boiler - ø850" | element type "09.Boiler - ø850" | 1 occurrence
  IFCBOILERTYPE "12. Temperature sensor" | element type "12. Temperature sensor" | 1 occurrence
  IFCBOILERTYPE "11. BCF 80-100-120 - Chimney Pipe" | element type "11. BCF 80-100-120 - Chimney Pipe" | 1 occurrence
  IFCBOILERTYPE "07. Condensation drainage (internal)" | element type "07. Condensation drainage (internal)" | 1 occurrence

Property sets
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = 1 (IFCINTEGER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = 0 (IFCINTEGER)
  Constraints | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Host = "Level : Level 1" (IFCLABEL)
    Level = "Level: Level 1" (IFCLABEL)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Host = "Level : Level 1" (IFCLABEL)
    Level = "Level: Level 1" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 100. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Host = "Level : Level 1" (IFCLABEL)
    Level = "Level: Level 1" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = -142.279425000005 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Host = "Level : Level 1" (IFCLABEL)
    Level = "Level: Level 1" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 226.783037026766 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Host = "Level : Level 1" (IFCLABEL)
    Level = "Level: Level 1" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 116.613466520526 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Mechanical | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    System Classification = "Domestic Hot Water,Domestic Cold Water,Other,Domestic Cold Water,Domestic Hot Water" (IFCLABEL)
    System Name = "" (IFCLABEL)
  Mechanical | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    APS Pressure < = 64.008 (IFCREAL)
  Identity Data | properties | on 2 objects (2 IFCENERGYCONVERSIONDEVICE)
    Assembly Code = "" (IFCLABEL)
    Assembly Description = "" (IFCLABEL)
    OmniClass Number = "" (IFCLABEL)
    OmniClass Title = "" (IFCLABEL)
  Identity Data | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Mark = "1" (IFCLABEL)
  Identity Data | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Assembly Code = "" (IFCLABEL)
    Assembly Description = "" (IFCLABEL)
    Manufacturer = "A.O. Smith" (IFCLABEL)
    OmniClass Number = "" (IFCLABEL)
    OmniClass Title = "" (IFCLABEL)
    Type Comments = "Condensation drainage (interna" (IFCLABEL)
  Identity Data | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Mark = "2" (IFCLABEL)
  Identity Data | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Mark = "3" (IFCLABEL)
  Identity Data | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Mark = "4" (IFCLABEL)
  Identity Data | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Mark = "5" (IFCLABEL)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCLABEL)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data: 3 more contents on 3 objects not shown
  Other | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Workspace = TRUE (IFCBOOLEAN)
  Other | properties | on 1 object (1 IFCBUILDING)
    Client Name = "Owner" (IFCLABEL)
    Project Address = "Enter address here" (IFCLABEL)
    Project Issue Date = "Issue Date" (IFCLABEL)
    Project Name = "Project Name" (IFCLABEL)
    Project Number = "Project Number" (IFCLABEL)
    Project Status = "Project Status" (IFCLABEL)
  Phasing | properties | on 5 objects (5 IFCENERGYCONVERSIONDEVICE)
    Phase Created = "New Construction" (IFCLABEL)
  Dimensions | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    A = 1960. (IFCLENGTHMEASURE) [MILLI METRE]
    K = 1616. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Diameter = 850. (IFCLENGTHMEASURE) [MILLI METRE]
    Flue Diameter - concentric system = "130/200 mm/mm" (IFCLABEL)
    Flue Diameter - parallel system = 130. (IFCLENGTHMEASURE) [MILLI METRE]
    Flue Diameter - water heater = "130/200 mm/mm" (IFCLABEL)
    Height = 2060. (IFCLENGTHMEASURE) [MILLI METRE]
    Height Air Inlet = 1995. (IFCLENGTHMEASURE) [MILLI METRE]
    Height Cold water Intlet = 225. (IFCLENGTHMEASURE) [MILLI METRE]
    Height Flue Outlet = 1995. (IFCLENGTHMEASURE) [MILLI METRE]
    Height Gas Connection = 1855. (IFCLENGTHMEASURE) [MILLI METRE]
    Height Warm Water Outlet = 2060. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 900. (IFCLENGTHMEASURE) [MILLI METRE]
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Mechanical - Flow | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Draw-off Capacity @ ΔT = 28°C after 120 min. = 197.762133640336 (IFCREAL)
    Draw-off Capacity @ ΔT = 28°C after 30 min. = 60.0349334265306 (IFCREAL)
    Draw-off Capacity @ ΔT = 28°C after 60 min. = 105.944000164466 (IFCREAL)
    Draw-off Capacity @ ΔT = 28°C after 90 min. = 151.853066902401 (IFCREAL)
    Draw-off Capacity @ ΔT = 44°C after 120 min. = 123.60133352521 (IFCREAL)
    Draw-off Capacity @ ΔT = 44°C after 30 min. = 33.1957867181993 (IFCREAL)
    Draw-off Capacity @ ΔT = 44°C after 60 min. = 63.5664000986795 (IFCREAL)
    Draw-off Capacity @ ΔT = 44°C after 90 min. = 91.8181334758703 (IFCREAL)
    Draw-off Capacity @ ΔT = 50°C after 120 min. = 105.944000164466 (IFCREAL)
    Draw-off Capacity @ ΔT = 50°C after 30 min. = 27.5454400427611 (IFCREAL)
    Draw-off Capacity @ ΔT = 50°C after 60 min. = 56.5034667543817 (IFCREAL)
    Draw-off Capacity @ ΔT = 50°C after 90 min. = 81.2237334594237 (IFCREAL)
    Draw-off Capacity @ ΔT = 55°C after 120 min. = 95.3496001480192 (IFCREAL)
    Draw-off Capacity @ ΔT = 55°C after 30 min. = 23.6608267033974 (IFCREAL)
    Draw-off Capacity @ ΔT = 55°C after 60 min. = 49.440533410084 (IFCREAL)
    Draw-off Capacity @ ΔT = 55°C after 90 min. = 70.6293334429772 (IFCREAL)
    Draw-off Capacity @ ΔT = 70°C after 120 min. = 0. (IFCREAL)
    Draw-off Capacity @ ΔT = 70°C after 30 min. = 0. (IFCREAL)
    Draw-off Capacity @ ΔT = 70°C after 60 min. = 0. (IFCREAL)
    Draw-off Capacity @ ΔT = 70°C after 90 min. = 0. (IFCREAL)
    Heating Up Time @ ΔT = 28°C = "11" (IFCLABEL)
    Heating Up Time @ ΔT = 44°C = "17" (IFCLABEL)
    Heating Up Time @ ΔT = 50°C = "20" (IFCLABEL)
    Heating Up Time @ ΔT = 55°C = "22" (IFCLABEL)
    Heating Up Time @ ΔT = 70°C = "0" (IFCLABEL)
    Recovery Rate @ ΔT = 28°C = 0. (IFCREAL)
    Recovery Rate @ ΔT = 44°C = 91.8181334758703 (IFCREAL)
    Recovery Rate @ ΔT = 50°C = 60.0349334265306 (IFCREAL)
    Recovery Rate @ ΔT = 55°C = 52.9720000822329 (IFCREAL)
    Recovery Rate @ ΔT = 70°C = 49.440533410084 (IFCREAL)
  General | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    1e Maintenance (check-up) = "3 months after installation" (IFCLABEL)
    2nd Maintenance (general maintenance) = "12 months after installation" (IFCLABEL)
    Maintenance Interval = "12 months" (IFCLABEL)
    Packaging Height = 2060. (IFCLENGTHMEASURE) [MILLI METRE]
    Packaging Length = 1020. (IFCLENGTHMEASURE) [MILLI METRE]
    Packaging Width = 920. (IFCLENGTHMEASURE) [MILLI METRE]
    Transport Weight = 491. (IFCREAL)
    Type of Packaging = "Plastic Shrink Wrap, Cardboard and Wood" (IFCLABEL)
    Warranty on parts = "12 months" (IFCLABEL)
    Warranty on tank = "36 months" (IFCLABEL)
  Model Properties | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Co2 Emissions (tol. +/- 1.0) vol% = "8.9" (IFCLABEL)
    Default Setpoint = 338.15 (IFCREAL)
    Empty Weight = 480. (IFCREAL)
    Gas Flow Rate - Mass kg/h = 0. (IFCREAL)
    Gas Flow Rate - Volume ltr/hr = 8.3 (IFCREAL)
    Insulation Thickness = 44. (IFCLENGTHMEASURE) [MILLI METRE]
    Max. Flue Gas Outlet Temperature = 323.15 (IFCREAL)
    Max. Operating Pressure = 243840. (IFCREAL)
    Max. Setpoint = 353.15 (IFCREAL)
    Min. Setpoint = 313.15 (IFCREAL)
    Noice-level dB (A) = "45" (IFCLABEL)
    Nominal Heat Input (Gross) = 932154.642087062 (IFCREAL)
    Nominal Heat Input (Net) = 839585.012503358 (IFCREAL)
    Nominal Output = 906321.257086959 (IFCREAL)
    Operating Weight = 960. (IFCREAL)
    Stand-by Loss - daily (24h) = 0. (IFCREAL)
    Stand-by Loss = 0. (IFCREAL)
    Storage Capacity = 16.9510400263145 (IFCREAL)
    Supply Pressure = 609.6 (IFCREAL)
  Plumbing | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Cold Water Connection R = 0.125 (IFCREAL)
    Condens Discharge Connection = 40. (IFCLENGTHMEASURE) [MILLI METRE]
    Drain Valve Connection Rp = 0.0625 (IFCREAL)
    Gas Connection R = 0.0625 (IFCREAL)
    Hot / Warm Water Connection R = 0.125 (IFCREAL)
    T&P Connection Rp = 0.0833333333333333 (IFCREAL)
  Energy Analysis | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Energy Efficiency Rating (Hi, acc NEN-EN 89-1999) = 108. (IFCREAL)
    Energy Efficiency Rating (Hs, acc NEN-EN 89-1999) = 97. (IFCREAL)
    Seasonal Energy Efficiency Rating = 97. (IFCREAL)
  Electrical | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    (Additional Control) Frequency = 50. (IFCREAL)
    (Additional Control) Phase = 1 (IFCINTEGER)
    (Additional Control) Power Consumption (nominal) = 7534.73729169681 (IFCREAL)
    (Additional Control) Voltage = 2475.69939584324 (IFCREAL)
    Frequency = 50. (IFCREAL)
    Phase = 1 (IFCINTEGER)
    Power Consumption (nominal) = 1022.57148958742 (IFCREAL)
    Voltage = 2475.69939584324 (IFCREAL)
  Green Building Properties | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    NOx Emissions (air free, 0% O2) ppm = "31" (IFCLABEL)
    NOx Emissions mg/kWh = "56" (IFCLABEL)