IFC building model
Schema: "IFC4"
Description: "ViewDefinition [CoordinationView_V2.0]"
Time stamp: "2018-02-28T14:39:01"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20170117_1200(x64) - Exporter 16.0.1205.0 - Default UI"
Application: "Autodesk Revit 2016 (ENU)" version "2016" identifier "Revit" by Organization "Autodesk Revit 2016 (ENU)"

People and organizations
  Person "michele.mollet@cadcompany.nl" of Organization (no name given)
  Owner history of Person "michele.mollet@cadcompany.nl" of Organization (no name given) | application "Autodesk Revit 2016 (ENU)" version "2016" identifier "Revit" by Organization "Autodesk Revit 2016 (ENU)" | change NOCHANGE | created 1519825136 (2018-02-28T13:38:56Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  PRESSUREUNIT: PASCAL

Spatial structure
IFCPROJECT | long name "C:\Users\mmt\Documents\01_Bestanden\01_Structure\Klanten\xxxxxxx - A.O. Smith 2018\In progress\Indirect-Water-Heater_AO_Smith-IT-1500_B.ifc"
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 3 elements
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Indirect-Water-Heater_AO_Smith-IT-1500_B" | object type "Indirect-Water-Heater_AO_Smith-IT-1500_B" | names: "Indirect-Water-Heater_AO_Smith-IT-1500_B:Indirect-Water-Heater_AO_Smith-IT-1500_B:10289" | material: materials ("RAL 9005", "Ral 9006 - Insulation", "Ral 9016") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Constraints, Dimensions, Identity Data, Mechanical
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "R1" | object type "R1" | names: "Warm water:R1:10290" | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Workspace" | object type "Workspace" | names: "Workspace:Workspace:10291" | material: "Workspace" | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Other, Phasing

Types
  IFCBUILDINGELEMENTPROXYTYPE "Indirect-Water-Heater_AO_Smith-IT-1500_B" | 1 occurrence | material: materials ("RAL 9005", "Ral 9006 - Insulation", "Ral 9016") | property sets: Dimensions, General, Identity Data, Mechanical - Flow, Model Properties, Other
  IFCBUILDINGELEMENTPROXYTYPE "R1" | 1 occurrence | property sets: Identity Data, Other
  IFCBUILDINGELEMENTPROXYTYPE "Workspace" | 1 occurrence | material: "Workspace" | property sets: Identity Data, Other

Property sets
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Mechanical Equipment" (IFCLABEL)
    Family = "Indirect-Water-Heater_AO_Smith-IT-1500_B: Indirect-Water-Heater_AO_Smith-IT-1500_B" (IFCLABEL)
    Family and Type = "Indirect-Water-Heater_AO_Smith-IT-1500_B: Indirect-Water-Heater_AO_Smith-IT-1500_B" (IFCLABEL)
    Type = "Indirect-Water-Heater_AO_Smith-IT-1500_B: Indirect-Water-Heater_AO_Smith-IT-1500_B" (IFCLABEL)
    Type Id = "Indirect-Water-Heater_AO_Smith-IT-1500_B: Indirect-Water-Heater_AO_Smith-IT-1500_B" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Mechanical Equipment" (IFCLABEL)
    Family = "Warm water: R1" (IFCLABEL)
    Family and Type = "Warm water: R1" (IFCLABEL)
    Type = "Warm water: R1" (IFCLABEL)
    Type Id = "Warm water: R1" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Generic Models" (IFCLABEL)
    Family = "Workspace: Workspace" (IFCLABEL)
    Family and Type = "Workspace: Workspace" (IFCLABEL)
    Type = "Workspace: Workspace" (IFCLABEL)
    Type Id = "Workspace: Workspace" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Level 1" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level: Level 1" (IFCLABEL)
    Type Id = "Level: Level 1" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Mechanical Equipment" (IFCLABEL)
    Family Name = "Indirect-Water-Heater_AO_Smith-IT-1500_B" (IFCTEXT)
  Other | properties | on 1 type object
    Category = "Mechanical Equipment" (IFCLABEL)
    Family Name = "Warm water" (IFCTEXT)
  Other: 1 more content on 0 objects not shown
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Indirect-Water-Heater_AO_Smith-IT-1500_B" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "R1" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Workspace" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Manufacturer = "A.O. Smith Water Products Company b.v." (IFCLABEL)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Host = "None" (IFCTEXT)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Host = "None" (IFCTEXT)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 1985. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Host = "None" (IFCTEXT)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 14.615004023204 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 2.6373807421061 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 0.0326151066195447 (IFCAREAMEASURE) [SQUARE_METRE]
    Diameter = 600. (IFCLENGTHMEASURE) [MILLI METRE]
    R = 63.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.00126670857252671 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 38.1893062744199 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 49.6105708441788 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Workspace Diameter = 2300. (IFCLENGTHMEASURE) [MILLI METRE]
    workspace_height = 2985. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    Diamètre (avec Isolation) = 1300. (IFCLENGTHMEASURE) [MILLI METRE]
    Diamètre (sans Isolation) = 1100. (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur (avec Isolation) = 1985. (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur (sans Isolation) = 1985. (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur de l'Alimentation en eau Froide = 135. (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur de la Sortie d'eau Chaude = 1985. (IFCLENGTHMEASURE) [MILLI METRE]
    Workspace Diameter = 2300. (IFCLENGTHMEASURE) [MILLI METRE]
    Workspace Height = 2985. (IFCLENGTHMEASURE) [MILLI METRE]
    espace de travail = 1100. (IFCLENGTHMEASURE) [MILLI METRE]
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Mark = "1" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Mark = "2" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "D3010" (IFCTEXT)
    Assembly Description = "Energy Supply" (IFCTEXT)
    BIM Content Developer = "CAD & Company" (IFCTEXT)
    BIM Content Developer URL = "http://www.cadcompany.nl/" (IFCTEXT)
    CE-PIN = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "Cuve Indirects Fournis d’un Échangeur" (IFCTEXT)
    Destination / Pays = "Belgique" (IFCTEXT)
    Fabricant No. = "E 7110" (IFCTEXT)
    Guide de Produit = "https://www.aosmithinternational.com/wp-content/uploads/Manuel-d-installation_IT-1500-3000_BEFR.pdf" (IFCTEXT)
    Manufacturer = "A.O. Smith Water Products Company b.v." (IFCTEXT)
    Model = "IT 1500 B" (IFCTEXT)
    Nombre de modèle du produit (EAN) = "8717449273347" (IFCTEXT)
    OmniClass Number = "23.75.00.00" (IFCTEXT)
    OmniClass Title = "Climate Control (HVAC)" (IFCTEXT)
    Spécifications du Produit = "https://www.aosmithinternational.com/wp-content/uploads/Feuille-technique_IT_BEFR.pdf" (IFCTEXT)
    Type Name = "Indirect-Water-Heater_AO_Smith-IT-1500_B" (IFCTEXT)
    URL = "https://www.aosmithinternational.com/be-fr/" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    Type Name = "R1" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    Type Name = "Workspace" (IFCTEXT)
  Mechanical | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    System Classification = "Hydronic Supply" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Phasing | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
    Reference = "Project Information" (IFCIDENTIFIER)
  General | properties | on 1 type object
    1er Entretien (check-up) = "3 mois après l'installation" (IFCTEXT)
    2ème Entretien (Entretien Général) = "12 mois après l'installation" (IFCTEXT)
    Garantie Pièces = "12 mois" (IFCTEXT)
    Garantie sur la Cuve = "36 mois" (IFCTEXT)
    Hauteur d'Emballage = 2060. (IFCLENGTHMEASURE) [MILLI METRE]
    Largeur d'Emballage = 1170. (IFCLENGTHMEASURE) [MILLI METRE]
    Poids de Transport = 488. (IFCREAL)
    Profondeur d'Emballage = 1426. (IFCLENGTHMEASURE) [MILLI METRE]
    Type d'Emballage = "Plastique et Bois" (IFCTEXT)
    l'Intervalle d'Entretien = "12 mois" (IFCTEXT)
  Mechanical - Flow | properties | on 1 type object
    Débit de vidage en Continu à ΔT = 28°C = 4454. (IFCREAL)
    Débit de vidage en Continu à ΔT = 44°C = 2834. (IFCREAL)
    Débit de vidage en Continu à ΔT = 50°C = 2494. (IFCREAL)
    Débit de vidage en Continu à ΔT = 55°C = 2267. (IFCREAL)
    Débit de vidage en Continu à ΔT = 70°C = 1781. (IFCREAL)
    Débit de vidage à ΔT = 28°C après 120 min. = 10.699 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Débit de vidage à ΔT = 28°C après 30 min. = 4.018 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Débit de vidage à ΔT = 28°C après 60 min. = 6.245 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Débit de vidage à ΔT = 28°C après 90 min. = 8.472 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Débit de vidage à ΔT = 44°C après 120 min. = 6.808 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Débit de vidage à ΔT = 44°C après 30 min. = 2.557 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Débit de vidage à ΔT = 44°C après 60 min. = 3.974 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Débit de vidage à ΔT = 44°C après 90 min. = 5.391 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Débit de vidage à ΔT = 50°C après 120 min. = 5.991 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Débit de vidage à ΔT = 50°C après 30 min. = 2.25 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Débit de vidage à ΔT = 50°C après 60 min. = 3.497 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Débit de vidage à ΔT = 50°C après 90 min. = 4.744 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Débit de vidage à ΔT = 55°C après 120 min. = 5.447 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Débit de vidage à ΔT = 55°C après 30 min. = 2.046 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Débit de vidage à ΔT = 55°C après 60 min. = 3.179 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Débit de vidage à ΔT = 55°C après 90 min. = 4.313 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Débit de vidage à ΔT = 70°C après 120 min. = 4.279 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Débit de vidage à ΔT = 70°C après 30 min. = 1.607 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Débit de vidage à ΔT = 70°C après 60 min. = 2.498 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Débit de vidage à ΔT = 70°C après 90 min. = 3.389 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Temps de réchauffement à ΔT = 28°C = "14" (IFCTEXT)
    Temps de réchauffement à ΔT = 44°C = "21" (IFCTEXT)
    Temps de réchauffement à ΔT = 50°C = "24" (IFCTEXT)
    Temps de réchauffement à ΔT = 55°C = "27" (IFCTEXT)
    Temps de réchauffement à ΔT = 70°C = 34 (IFCINTEGER)
  Model Properties | properties | on 1 type object
    Capacité - Cuve = 1550. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Capacité - Échangeur Inférieur = 40. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Charge Maximale au Sol = 1948. (IFCREAL)
    Débit à 80ºC/60ºC - Échangeur Inférieur = 6485. (IFCREAL)
    Epaisseur d'Isolation = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    Max. Température de l'eau - Réservoir = 85. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Niveau du Son = "0" (IFCTEXT)
    Perte de Pression à 80ºC/60ºC - Échangeur Inférieur = 830000. (IFCPRESSUREMEASURE) [PASCAL]
    Pertes en Veille - tous les jours (24h) = 0. (IFCREAL)
    Pertes en Veille = 0. (IFCPOWERMEASURE) [WATT]
    Poids à vide = 398. (IFCREAL)
    Pression de Service Maximale - Réservoir = 80000. (IFCPRESSUREMEASURE) [PASCAL]
    Pression de Service Maximale - Échangeur Inférieur = 60000. (IFCPRESSUREMEASURE) [PASCAL]
    Production Nominale - Échangeur Inférieur = 147000. (IFCPOWERMEASURE) [WATT]
    Surface d'Échange de Chaleur - Échangeur Inférieur = 5.2 (IFCAREAMEASURE) [SQUARE_METRE]
    Température Maximale - Échangeur Inférieur = 90. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Plumbing | properties | on 1 type object
    Raccord d'Alimentation en Eau Froide = 50.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Raccord de Sortie d'Eau Chaude = 50.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Raccord de la Soupape de Vidange = 25.4 (IFCLENGTHMEASURE) [MILLI METRE]