IFC building model
Schema: "IFC4"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "0001"
Time stamp: "2016-11-04T16:16:41"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20160512_0715(x64) - Exporter 15.7.0.0 - Default UI"
Application: "Autodesk Revit 2015 (ENU)" version "2015" identifier "Revit" by Organization "Autodesk Revit 2015 (ENU)"

People and organizations
  Person "michele.mollet@cadcompany.nl" of Organization (no name given)
  Owner history of Person "michele.mollet@cadcompany.nl" of Organization (no name given) | application "Autodesk Revit 2015 (ENU)" version "2015" identifier "Revit" by Organization "Autodesk Revit 2015 (ENU)" | change NOCHANGE | created 1478272598 (2016-11-04T15:16:38Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "0001" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 30.344238″ | longitude -71° 3′ 35.194702″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "<Default>"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 2 elements
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "IR-24-245 BEFR LP" | object type "IR-24-245 BEFR LP" | names: "Innovo BEFR_IR 24 245 BEFR LP:IR-24-245 BEFR LP:271349" | material: materials ("Rubber", "Aluminium", "RAL 9006", "RAL 9005", "display", "RAL 9011") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Constraints, Dimensions, Identity Data, Mechanical
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Workspace" | object type "Workspace" | names: "Innovo_workspace:Workspace:271352" | material: "Workspace 3D" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Constraints, Dimensions, Identity Data, Other

Types
  IFCBUILDINGELEMENTPROXYTYPE "IR-24-245 BEFR LP" | 1 occurrence | material: materials ("Rubber", "Aluminium", "RAL 9006", "RAL 9005", "display", "RAL 9011") | property sets: Constraints(Type), Dimensions(Type), Electrical(Type), Energy Analysis(Type), General(Type), Green Building Properties(Type)
  IFCBUILDINGELEMENTPROXYTYPE "Workspace" | 1 occurrence | material: "Workspace 3D" | property sets: Identity Data(Type), Other(Type)

Property sets
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other(Type) | properties | on 1 type object
    Category = "Mechanical Equipment" (IFCLABEL)
    Family Name = "Innovo BEFR_IR 24 245 BEFR LP" (IFCTEXT)
    Workspace Front Distance = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    Workspace Height = 2545. (IFCLENGTHMEASURE) [MILLI METRE]
    Workspace Radius = 780. (IFCLENGTHMEASURE) [MILLI METRE]
  Other(Type) | properties | on 1 type object
    Category = "Mechanical Equipment" (IFCLABEL)
    Family Name = "Innovo_workspace" (IFCTEXT)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "0001" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Mechanical Equipment" (IFCLABEL)
    Family = "Innovo BEFR_IR 24 245 BEFR LP: IR-24-245 BEFR LP" (IFCLABEL)
    Family and Type = "Innovo BEFR_IR 24 245 BEFR LP: IR-24-245 BEFR LP" (IFCLABEL)
    Type = "Innovo BEFR_IR 24 245 BEFR LP: IR-24-245 BEFR LP" (IFCLABEL)
    Type Id = "Innovo BEFR_IR 24 245 BEFR LP: IR-24-245 BEFR LP" (IFCLABEL)
    Workspace = TRUE (IFCBOOLEAN)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Mechanical Equipment" (IFCLABEL)
    Family = "Innovo_workspace: Workspace" (IFCLABEL)
    Family and Type = "Innovo_workspace: Workspace" (IFCLABEL)
    Type = "Innovo_workspace: Workspace" (IFCLABEL)
    Type Id = "Innovo_workspace: Workspace" (IFCLABEL)
    Workspace = TRUE (IFCBOOLEAN)
    Workspace Distance Front = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    Workspace Height = 2545. (IFCLENGTHMEASURE) [MILLI METRE]
    Workspace Radius = 780. (IFCLENGTHMEASURE) [MILLI METRE]
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8mm Head" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "Level: 8mm Head" (IFCLABEL)
    Type Id = "Level: 8mm Head" (IFCLABEL)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Identity Data(Type) | properties | on 1 type object
    Assembly Code = "D3010" (IFCTEXT)
    Assembly Description = "Energy Supply" (IFCTEXT)
    BIM Content Developer = "CAD & Company" (IFCTEXT)
    CE-PIN = "0063CQ3037" (IFCTEXT)
    Catégorie de Gaz = "I3P" (IFCTEXT)
    Created By = "http://www.cadcompany.nl/" (IFCTEXT)
    Description = "Préparateur ECS Solaire en Combinaison avec Réservoir de Stockage" (IFCTEXT)
    Destination / Country = "Belgique" (IFCTEXT)
    Fabricant No. = "E 7110" (IFCTEXT)
    Guide de Produit = "" (IFCTEXT)
    Manufacturer = "A.O. Smith Water Products Company b.v." (IFCTEXT)
    Model = "IR-24-245 FR LP" (IFCTEXT)
    Nombre de modèle du produit (EAN) = "8717449286149" (IFCTEXT)
    OmniClass Number = "23.75.00.00" (IFCTEXT)
    OmniClass Title = "Climate Control (HVAC)" (IFCTEXT)
    Réglage Standard Pour = "G31" (IFCTEXT)
    Spécifications du Produit = "" (IFCTEXT)
    Type Name = "IR-24-245 BEFR LP" (IFCTEXT)
    Type d'Installation = "B23/C13/C33/C43/C53/C63" (IFCTEXT)
    URL = "www.aosmith.be" (IFCTEXT)
  Identity Data(Type) | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    BIM Content Developer = "CAD & Company" (IFCTEXT)
    Created By = "" (IFCTEXT)
    Description = "" (IFCTEXT)
    Manufacturer = "A.O. Smith Water Products Company b.v." (IFCTEXT)
    Model = "" (IFCTEXT)
    OmniClass Number = "23.75.00.00" (IFCTEXT)
    OmniClass Title = "Climate Control (HVAC)" (IFCTEXT)
    Type Name = "Workspace" (IFCTEXT)
    URL = "www.aosmith.nl" (IFCTEXT)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Mark = "1" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Mark = "2" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Constraints(Type) | properties | on 1 type object
    Valve Height 01 = 693. (IFCLENGTHMEASURE) [MILLI METRE]
    Valve Height 02 = 1328. (IFCLENGTHMEASURE) [MILLI METRE]
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "IR-24-245 BEFR LP" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Workspace" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Manufacturer = "A.O. Smith Water Products Company b.v." (IFCLABEL)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Host = "None" (IFCTEXT)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Host = "None" (IFCTEXT)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 3.28085598836932 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.535844922894665 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 10.2565617478661 (IFCAREAMEASURE) [SQUARE_METRE]
    Center to Front = 517.825381227623 (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 5.89944166666002 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Mechanical | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    System Classification = "Domestic Hot Water,Other Air" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Phasing | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Phase Created = "Phase 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
    Reference = "Project Information" (IFCIDENTIFIER)
  Dimensions(Type) | properties | on 1 type object
    Diameter = 610. (IFCLENGTHMEASURE) [MILLI METRE]
    Diamètre Cheminée - Boiler = "80/125 mm/mm" (IFCTEXT)
    Diamètre Cheminée - Système Concentrique = "80/125 mm/mm" (IFCTEXT)
    Diamètre Cheminée - Système Parallèle = "2x80" (IFCTEXT)
    Hauteur = 1545. (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur Conduit d'Alimentation en Air = 1345. (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur Conduit d'Évacuation des Fumées = 1345. (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur de l'Alimentation en eau Froide = 170. (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur de la Sortie d'eau Chaude = 1545. (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur du Raccordement au Gaz = 920. (IFCLENGTHMEASURE) [MILLI METRE]
    Largeur = 610. (IFCLENGTHMEASURE) [MILLI METRE]
    Profondeur = 780. (IFCLENGTHMEASURE) [MILLI METRE]
  Electrical(Type) | properties | on 1 type object
    Fréquence secteur = 50. (IFCFREQUENCYMEASURE) [HERTZ]
    Phase = 1 (IFCINTEGER)
    Puissance Électrique Absorbée (nominal) = 51. (IFCPOWERMEASURE) [WATT]
    Puissance Électrique Absorbée (sommet) = 105. (IFCPOWERMEASURE) [WATT]
    Tension d'Alimentation (-15%, +10%) = 230. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
  Energy Analysis(Type) | properties | on 1 type object
    Annual electricity consumption (1) = "42 kWh" (IFCTEXT)
    Annual electricity consumption (2) = "-" (IFCTEXT)
    Annual fuel consumption (1) = "21 GJ GCV" (IFCTEXT)
    Annual fuel consumption (2) = "-" (IFCTEXT)
    Class d'efficacité énergétique (1) = "A" (IFCTEXT)
    Class d'efficacité énergétique (2) = "-" (IFCTEXT)
    D'autres profils de soutirage = "-" (IFCTEXT)
    Forctionner qu'en heures creuses = FALSE (IFCBOOLEAN)
    L'efficacité énergétique pour le chauffage de l'eau (1) = "92%" (IFCTEXT)
    L'efficacité énergétique pour le chauffage de l'eau (2) = "-" (IFCTEXT)
    La commande intelligente = FALSE (IFCBOOLEAN)
    Marque commerciale = "A.O. Smith" (IFCTEXT)
    Modèdele = "IR-24-285" (IFCTEXT)
    Niveau de puissance acoustique à l'intérieur = "53 dB" (IFCTEXT)
    Precaustions during assembling, installation or maintenance = "voir Manuel d'installation, d'emploi er d'entretien" (IFCTEXT)
    Profils de soutirage déclaré = "XXL" (IFCTEXT)
    Rendement (Hi, acc. NEN-EN 89 - 1999) = 107. (IFCREAL)
    Rendement (Hs, acc. NEN-EN 89 - 1999) = 96. (IFCREAL)
    Rendement Saisonnier (Hs) = 96. (IFCREAL)
    Réglages du thermostat du chauffe-eau = 65. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  General(Type) | properties | on 1 type object
    1er Entretien (check-up) = "3 mois après l'installation" (IFCTEXT)
    2ème Entretien (Entretien Général) = "12 mois après l'installation" (IFCTEXT)
    Garantie Pièces = "12 mois" (IFCTEXT)
    Garantie sur la Cuve = "36 mois" (IFCTEXT)
    Hauteur d'emballage = 1695. (IFCLENGTHMEASURE) [MILLI METRE]
    Poids de Transport = 136. (IFCREAL)
    Profondeur d'emballage = 946. (IFCLENGTHMEASURE) [MILLI METRE]
    Type d'emballage = "Carton et bois" (IFCTEXT)
    l'Intervalle d'Entretien = "12 mois" (IFCTEXT)
    largeur d'emballage = 786. (IFCLENGTHMEASURE) [MILLI METRE]
  Green Building Properties(Type) | properties | on 1 type object
    NOx-émissions (ven air, 0% O2) ppm = "20" (IFCTEXT)
    NOx-émissions mg/kWh = "33" (IFCTEXT)
  Mechanical - Flow(Type) | properties | on 1 type object
    Débit de vidage en Continu à ΔT = 28°C = 25.7797067066867 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Débit de vidage en Continu à ΔT = 44°C = 16.2447466918848 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Débit de vidage en Continu à ΔT = 50°C = 14.1258666885954 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Débit de vidage en Continu à ΔT = 55°C = 13.0664266869508 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Débit de vidage en Continu à ΔT = 70°C = 10.2412533492317 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Débit de vidage à ΔT = 28°C après 120 min. = 0.2 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Débit de vidage à ΔT = 28°C après 30 min. = 0.83 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Débit de vidage à ΔT = 28°C après 60 min. = 1.2 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Débit de vidage à ΔT = 28°C après 90 min. = 1.6 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Débit de vidage à ΔT = 44°C après 120 min. = 1.2 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Débit de vidage à ΔT = 44°C après 30 min. = 0.51 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Débit de vidage à ΔT = 44°C après 60 min. = 0.74 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Débit de vidage à ΔT = 44°C après 90 min. = 0.97 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Débit de vidage à ΔT = 50°C après 120 min. = 1.1 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Débit de vidage à ΔT = 50°C après 30 min. = 0.44 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Débit de vidage à ΔT = 50°C après 60 min. = 0.64 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Débit de vidage à ΔT = 50°C après 90 min. = 0.84 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Débit de vidage à ΔT = 55°C après 120 min. = 0.94 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Débit de vidage à ΔT = 55°C après 30 min. = 0.39 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Débit de vidage à ΔT = 55°C après 60 min. = 0.57 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Débit de vidage à ΔT = 55°C après 90 min. = 0.76 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Débit de vidage à ΔT = 70°C après 120 min. = 0.72 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Débit de vidage à ΔT = 70°C après 30 min. = 0.28 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Débit de vidage à ΔT = 70°C après 60 min. = 0.43 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Débit de vidage à ΔT = 70°C après 90 min. = 0.57 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Temps de réchauffement à ΔT = 28°C = "16" (IFCTEXT)
    Temps de réchauffement à ΔT = 44°C = "25" (IFCTEXT)
    Temps de réchauffement à ΔT = 50°C = "29" (IFCTEXT)
    Temps de réchauffement à ΔT = 55°C = "32" (IFCTEXT)
    Temps de réchauffement à ΔT = 70°C = "40" (IFCTEXT)
  Mechanical(Type) | properties | on 1 type object
    Pression Différentielle d'Ouverture de l'Interrupteur de Pression < = 210. (IFCPRESSUREMEASURE) [PASCAL]
  Model Properties(Type) | properties | on 1 type object
    CO2 Émissions (tol. +/- 1.0) vol% = "10.0" (IFCTEXT)
    Capacité = 0.245 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Charge Maximale au Sol = 381. (IFCREAL)
    Charge Nominale (Valeur Inférieure) = "22000.0" (IFCTEXT)
    Charge Nominale (Valeur Supérieure) = "23900.0" (IFCTEXT)
    Consommation de Gaz - Masse kg/h = "1.7" (IFCTEXT)
    Consommation de Gaz - Volume ltr/hr = "a/p" (IFCTEXT)
    Epaisseur d'Isolation = 44. (IFCLENGTHMEASURE) [MILLI METRE]
    Niveau du Son dB (A) = "<45" (IFCTEXT)
    Pertes en Veille - tous les jours (24h) = 0. (IFCPOWERMEASURE) [WATT]
    Pertes en Veille = 0. (IFCPOWERMEASURE) [WATT]
    Poids à vide = 120. (IFCREAL)
    Pression Amont de Gaz = "3700 Pa" (IFCTEXT)
    Pression de Fonctionnement Maximale = 800000. (IFCPRESSUREMEASURE) [PASCAL]
    Production Nominale = "23000.0" (IFCTEXT)
    Température Maximale des Fumées = 57. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Valeur Défaut du Thermostat de Régulation = 65. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Valeur Manimale du Thermostat de Régulation = 40. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Valeur Maximale du Thermostat de Régulation = 85. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
  Plumbing(Type) | properties | on 1 type object
    Raccord Robinet de Vidange = 19.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Raccord d'Alimentation en Eau Froide = 19.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Raccord de Gaz = 381. (IFCLENGTHMEASURE) [MILLI METRE]
    Raccord de Sortie d'Eau Chaude = 25.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Raccord de la Soupape de Vidange = 25.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Raccord Évacuation de la Condensation = 40. (IFCLENGTHMEASURE) [MILLI METRE]