IFC building model
Schema: "IFC4"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "0001"
Time stamp: "2016-11-09T11:05:56"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20160512_0715(x64) - Exporter 15.7.0.0 - Default UI"
Application: "Autodesk Revit 2015 (ENU)" version "2015" identifier "Revit" by Organization "Autodesk Revit 2015 (ENU)"

People and organizations
  Person "michele.mollet@cadcompany.nl" of Organization (no name given)
  Owner history of Person "michele.mollet@cadcompany.nl" of Organization (no name given) | application "Autodesk Revit 2015 (ENU)" version "2015" identifier "Revit" by Organization "Autodesk Revit 2015 (ENU)" | change NOCHANGE | created 1478685952 (2016-11-09T10:05:52Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "0001" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 30.344238″ | longitude -71° 3′ 35.194702″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "<Default>"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 2 elements
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "IR-32-245 GB LP" | object type "IR-32-245 GB LP" | names: "Innovo GB_IR 32 245 GB LP:IR-32-245 GB LP:271160" | material: materials ("Rubber", "Aluminium", "RAL 9006", "RAL 9005", "display", "RAL 9011") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Constraints, Dimensions, Identity Data, Mechanical
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Workspace" | object type "Workspace" | names: "Innovo_workspace:Workspace:271161" | material: "Workspace 3D" | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Constraints, Dimensions, Identity Data, Other

Types
  IFCBUILDINGELEMENTPROXYTYPE "IR-32-245 GB LP" | 1 occurrence | material: materials ("Rubber", "Aluminium", "RAL 9006", "RAL 9005", "display", "RAL 9011") | property sets: Constraints(Type), Dimensions(Type), Electrical(Type), Energy Analysis(Type), General(Type), Green Building Properties(Type)
  IFCBUILDINGELEMENTPROXYTYPE "Workspace" | 1 occurrence | material: "Workspace 3D" | property sets: Identity Data(Type), Other(Type)

Property sets
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other(Type) | properties | on 1 type object
    Category = "Mechanical Equipment" (IFCLABEL)
    Family Name = "Innovo GB_IR 32 245 GB LP" (IFCTEXT)
    Workspace Front Distance = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    Workspace Height = 2545. (IFCLENGTHMEASURE) [MILLI METRE]
    Workspace Radius = 780. (IFCLENGTHMEASURE) [MILLI METRE]
  Other(Type) | properties | on 1 type object
    Category = "Mechanical Equipment" (IFCLABEL)
    Family Name = "Innovo_workspace" (IFCTEXT)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "0001" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Mechanical Equipment" (IFCLABEL)
    Family = "Innovo GB_IR 32 245 GB LP: IR-32-245 GB LP" (IFCLABEL)
    Family and Type = "Innovo GB_IR 32 245 GB LP: IR-32-245 GB LP" (IFCLABEL)
    Type = "Innovo GB_IR 32 245 GB LP: IR-32-245 GB LP" (IFCLABEL)
    Type Id = "Innovo GB_IR 32 245 GB LP: IR-32-245 GB LP" (IFCLABEL)
    Workspace = TRUE (IFCBOOLEAN)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Mechanical Equipment" (IFCLABEL)
    Family = "Innovo_workspace: Workspace" (IFCLABEL)
    Family and Type = "Innovo_workspace: Workspace" (IFCLABEL)
    Type = "Innovo_workspace: Workspace" (IFCLABEL)
    Type Id = "Innovo_workspace: Workspace" (IFCLABEL)
    Workspace = TRUE (IFCBOOLEAN)
    Workspace Distance Front = 1000. (IFCLENGTHMEASURE) [MILLI METRE]
    Workspace Height = 2545. (IFCLENGTHMEASURE) [MILLI METRE]
    Workspace Radius = 780. (IFCLENGTHMEASURE) [MILLI METRE]
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8mm Head" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "Level: 8mm Head" (IFCLABEL)
    Type Id = "Level: 8mm Head" (IFCLABEL)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Identity Data(Type) | properties | on 1 type object
    Assembly Code = "D3010" (IFCTEXT)
    Assembly Description = "Energy Supply" (IFCTEXT)
    BIM Content Developer = "CAD & Company" (IFCTEXT)
    CE-PIN = "0063CQ3037" (IFCTEXT)
    Created By = "http://www.cadcompany.nl/" (IFCTEXT)
    Description = "Condensing High Efficiency Storage Water Heater" (IFCTEXT)
    Destination / Country = "UK & Ireland" (IFCTEXT)
    Gas Category = "II2E3P" (IFCTEXT)
    Installation Type = "B23/C13/C33/C43/C53/C63" (IFCTEXT)
    Manufacturer = "A.O. Smith Water Products Company b.v." (IFCTEXT)
    Manufacturer Number = "E 7110" (IFCTEXT)
    Model = "IR-32-325 GB LP" (IFCTEXT)
    OmniClass Number = "23.75.00.00" (IFCTEXT)
    OmniClass Title = "Climate Control (HVAC)" (IFCTEXT)
    Product Documentation Link = "" (IFCTEXT)
    Product Instruction Link = "" (IFCTEXT)
    Serial Number = "8717449286309" (IFCTEXT)
    Standard Set For = "G31" (IFCTEXT)
    Type Name = "IR-32-245 GB LP" (IFCTEXT)
    URL = "www.aosmith.co.uk" (IFCTEXT)
  Identity Data(Type) | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    BIM Content Developer = "CAD & Company" (IFCTEXT)
    Created By = "" (IFCTEXT)
    Description = "" (IFCTEXT)
    Manufacturer = "A.O. Smith Water Products Company b.v." (IFCTEXT)
    Model = "" (IFCTEXT)
    OmniClass Number = "23.75.00.00" (IFCTEXT)
    OmniClass Title = "Climate Control (HVAC)" (IFCTEXT)
    Type Name = "Workspace" (IFCTEXT)
    URL = "www.aosmith.nl" (IFCTEXT)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Mark = "1" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Mark = "2" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Constraints(Type) | properties | on 1 type object
    Valve Height 01 = 693. (IFCLENGTHMEASURE) [MILLI METRE]
    Valve Height 02 = 1328. (IFCLENGTHMEASURE) [MILLI METRE]
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "IR-32-245 GB LP" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Workspace" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Manufacturer = "A.O. Smith Water Products Company b.v." (IFCLABEL)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Host = "None" (IFCTEXT)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Host = "None" (IFCTEXT)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 3.28085598836932 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.535844922894665 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 10.2565617478661 (IFCAREAMEASURE) [SQUARE_METRE]
    Center to Front = 517.825381227623 (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 5.89944166666002 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Mechanical | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    System Classification = "Domestic Hot Water,Other Air" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Phasing | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Phase Created = "Phase 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
    Reference = "Project Information" (IFCIDENTIFIER)
  Dimensions(Type) | properties | on 1 type object
    Diameter = 610. (IFCLENGTHMEASURE) [MILLI METRE]
    Flue Diameter - concentric system = "80/125 mm/mm" (IFCTEXT)
    Flue Diameter - parallel system = "2x80" (IFCTEXT)
    Flue Diameter - water heater = "80/125 mm/mm" (IFCTEXT)
    Height = 1545. (IFCLENGTHMEASURE) [MILLI METRE]
    Height Air Inlet = 1345. (IFCLENGTHMEASURE) [MILLI METRE]
    Height Cold Water Inlet = 170. (IFCLENGTHMEASURE) [MILLI METRE]
    Height Flue Outlet = 1345. (IFCLENGTHMEASURE) [MILLI METRE]
    Height Gas Connection = 920. (IFCLENGTHMEASURE) [MILLI METRE]
    Height Warm Water Outlet = 1545. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 780. (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 610. (IFCLENGTHMEASURE) [MILLI METRE]
  Electrical(Type) | properties | on 1 type object
    Frequency = 50. (IFCFREQUENCYMEASURE) [HERTZ]
    Phase = 1 (IFCINTEGER)
    Power Consumption (nominal) = 85. (IFCPOWERMEASURE) [WATT]
    Power Consumption (peak) = 105. (IFCPOWERMEASURE) [WATT]
    Voltage = 230. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
  Energy Analysis(Type) | properties | on 1 type object
    Annual electricity consumption (1) = "44 kWh" (IFCTEXT)
    Annual electricity consumption (2) = "-" (IFCTEXT)
    Annual fuel consumption (1) = "21 GJ GCV" (IFCTEXT)
    Annual fuel consumption (2) = "-" (IFCTEXT)
    Energy Efficiency Rating (Hi, acc NEN-EN 89-1999) = 106. (IFCREAL)
    Energy Efficiency Rating (Hs, acc NEN-EN 89-1999) = 95. (IFCREAL)
    Indoor sound power level = "58 dB" (IFCTEXT)
    Load profile = "XXL" (IFCTEXT)
    Model identifier = "IR-32-245" (IFCTEXT)
    Other load profile = "-" (IFCTEXT)
    Precaustions during assembling, installation or maintenance = "see User, Installation, Service and Maintenance Manual" (IFCTEXT)
    Seasonal Energy Efficiency Rating = 95. (IFCREAL)
    Smart control = FALSE (IFCBOOLEAN)
    Thermostat temperature setting = 65. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Trade mark = "A.O. Smith" (IFCTEXT)
    Water heating energy efficiency (1) = "92%" (IFCTEXT)
    Water heating energy efficiency (2) = "-" (IFCTEXT)
    Water heating energy efficiency class (1) = "A" (IFCTEXT)
    Water heating energy efficiency class (2) = "-" (IFCTEXT)
    Working only during off-peak hour = FALSE (IFCBOOLEAN)
  General(Type) | properties | on 1 type object
    1e Maintenance (check-up) = "3 months after installation" (IFCTEXT)
    2nd Maintenance (general maintenance) = "12 months after installation" (IFCTEXT)
    Maintenance Interval = "12 months" (IFCTEXT)
    Packaging Height = 1695. (IFCLENGTHMEASURE) [MILLI METRE]
    Packaging Length = 946. (IFCLENGTHMEASURE) [MILLI METRE]
    Packaging Width = 786. (IFCLENGTHMEASURE) [MILLI METRE]
    Transport Weight = 136. (IFCREAL)
    Type of Packaging = "Carton and Wood" (IFCTEXT)
    Warranty on parts = "12 months" (IFCTEXT)
    Warranty on tank = "36 months" (IFCTEXT)
  Green Building Properties(Type) | properties | on 1 type object
    NOx Emissions (air free, 0% O2) ppm = "63.0/23.0" (IFCTEXT)
    NOx Emissions mg/kWh = "103.0/37.0" (IFCTEXT)
  Mechanical - Flow(Type) | properties | on 1 type object
    Draw-off Capacity @ ΔT = 28°C after 120 min. = 2.4 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 28°C after 30 min. = 0.93 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 28°C after 60 min. = 1.4 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 28°C after 90 min. = 1.9 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 44°C after 120 min. = 1.5 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 44°C after 30 min. = 0.57 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 44°C after 60 min. = 0.87 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 44°C after 90 min. = 1.2 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 50°C after 120 min. = 1.3 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 50°C after 30 min. = 0.5 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 50°C after 60 min. = 0.76 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 50°C after 90 min. = 1.1 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 55°C after 120 min. = 1.2 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 55°C after 30 min. = 0.44 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 55°C after 60 min. = 0.69 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 55°C after 90 min. = 0.93 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 70°C after 120 min. = 0.9 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 70°C after 30 min. = 0.33 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 70°C after 60 min. = 0.49 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 70°C after 90 min. = 0.71 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Heating Up Time @ ΔT = 28°C = "13" (IFCTEXT)
    Heating Up Time @ ΔT = 44°C = "20" (IFCTEXT)
    Heating Up Time @ ΔT = 50°C = "22" (IFCTEXT)
    Heating Up Time @ ΔT = 55°C = "24" (IFCTEXT)
    Heating Up Time @ ΔT = 70°C = "31" (IFCTEXT)
    Recovery Rate @ ΔT = 28°C = 33.902080052629 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Recovery Rate @ ΔT = 44°C = 21.1888000328932 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Recovery Rate @ ΔT = 50°C = 18.7167733623889 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Recovery Rate @ ΔT = 55°C = 16.9510400263145 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Recovery Rate @ ΔT = 70°C = 13.4195733541657 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
  Mechanical(Type) | properties | on 1 type object
    APS Pressure < = 210. (IFCPRESSUREMEASURE) [PASCAL]
  Model Properties(Type) | properties | on 1 type object
    Co2 Emissions (tol. +/- 1.0) vol% = "10" (IFCTEXT)
    Default Setpoint = 65. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Empty Weight = 120. (IFCREAL)
    Gas Flow Rate - Mass kg/h = "2.3" (IFCTEXT)
    Gas Flow Rate - Volume ltr/hr = "n.a." (IFCTEXT)
    Gas Supply Pressure = 3700. (IFCPRESSUREMEASURE) [PASCAL]
    Insulation Thickness = 44. (IFCLENGTHMEASURE) [MILLI METRE]
    Max. Flue Gas Outlet Temperature = 65. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Max. Operating Pressure = 800000. (IFCPRESSUREMEASURE) [PASCAL]
    Max. Setpoint = 85. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Min. Setpoint = 40. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Noice-level dB (A) = "<45" (IFCTEXT)
    Nominal Heat Input (Gross) = "31500" (IFCTEXT)
    Nominal Heat Input (Net) = "29000" (IFCTEXT)
    Nominal Output = "30100" (IFCTEXT)
    Operating Weight = 381. (IFCREAL)
    Stand-by Loss - daily (24h) = 0. (IFCPOWERMEASURE) [WATT]
    Stand-by Loss = 0. (IFCPOWERMEASURE) [WATT]
    Storage Capacity = 0.245 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Plumbing(Type) | properties | on 1 type object
    Cold Water Connection R = 19.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Condens Discharge Connection = 40. (IFCLENGTHMEASURE) [MILLI METRE]
    Drain Valve Connection Rp = 19.05 (IFCLENGTHMEASURE) [MILLI METRE]
    Gas Connection R = 381. (IFCLENGTHMEASURE) [MILLI METRE]
    Hot / Warm Water Connection R = 25.4 (IFCLENGTHMEASURE) [MILLI METRE]
    T&P Connection Rp = 25.4 (IFCLENGTHMEASURE) [MILLI METRE]