IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
File name: "0001"
Time stamp: "2015-05-08T13:47:11"
Preprocessor: "The EXPRESS Data Manager Version 5.01.0100.02.64mod : 6 Jun 2012"
Originating system: "20130308_1515(x64) - Exporter 2014.0.2013.0308 - Default UI"
Application: "Autodesk Revit 2014 (ENU)" version "2014" identifier "Revit" by Organization "Autodesk Revit 2014 (ENU)"

People and organizations
  Person "BTN" of Organization (no name given)
  Owner history of Person "BTN" of Organization (no name given) | application "Autodesk Revit 2014 (ENU)" version "2014" identifier "Revit" by Organization "Autodesk Revit 2014 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: KELVIN
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  POWERUNIT: WATT

Spatial structure
IFCPROJECT "0001" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 30.344238″ | longitude -71° 3′ 35.194702″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "<Default>"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 3 elements
          1 x IFCBUILDINGELEMENTPROXY | object type "Storage-Vessel_AO_Smith-ST-500_G_E" | names: "Storage-Vessel_AO_Smith-ST-500_G_E:Storage-Vessel_AO_Smith-ST-500_G_E:720279" | material: materials ("RAL 9005", "RAL 9017", "Ral 9006 - Insulation", "Ral 9016") | property sets: Mechanical, Identity Data, Constraints, Phasing, Pset_ManufacturerTypeInformation, Pset_BuildingElementProxyCommon
          1 x IFCBUILDINGELEMENTPROXY | object type "R1" | names: "Warm water:R1:720281" | property sets: Dimensions, Constraints, Phasing, Pset_BuildingElementProxyCommon, Identity Data
          1 x IFCBUILDINGELEMENTPROXY | object type "Workspace" | names: "Workspace:Workspace:720282" | material: "Workspace" | property sets: Dimensions, Identity Data, Constraints, Phasing, Pset_BuildingElementProxyCommon

Property sets
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 2010. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Mechanical | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    System Classification = "Hydronic Supply,Domestic Hot Water" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Identity Data | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Mark = "1" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCBUILDING)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Assembly Code = "D3010" (IFCTEXT)
    Assembly Description = "Energy Supply" (IFCTEXT)
    BIM Content Developer = "CAD & Company" (IFCTEXT)
    BIM Content Developer URL = "http:/www.cadcompany.nl" (IFCTEXT)
    CE-PIN = "" (IFCTEXT)
    Description = "Storage Vessel" (IFCTEXT)
    Destination / Counrty = "UK & Ireland" (IFCTEXT)
    Manufacturer = "A.O. Smith Water Products Company b.v." (IFCTEXT)
    Manufacturer Number = "E 7110 E 7110 E 7110" (IFCTEXT)
    Model = "ST 500 G E" (IFCTEXT)
    OmniClass Number = "23.75.00.00" (IFCTEXT)
    OmniClass Title = "Climate Control (HVAC)" (IFCTEXT)
    Product Documentation Link = "http://www.aosmithinternational.com/sites/aosmithinternational.com/files/PDF-NL/Specs-sheet-IT-NL.pdf" (IFCTEXT)
    Product Instruction Link = "http://www.aosmithinternational.com/sites/aosmithinternational.com/files/PDF-ALL/Instruction-manual-IT400-1000-NL-UK-FR.pdf" (IFCTEXT)
    Serial Number = "8717449179939" (IFCTEXT)
    URL = "www.aosmith.co.uk" (IFCTEXT)
  Phasing | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Manufacturer = "A.O. Smith Water Products Company b.v." (IFCLABEL)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Storage-Vessel_AO_Smith-ST-500_G_E" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "R1" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Workspace" (IFCIDENTIFIER)
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Workspace = 860. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Diameter = 360. (IFCLENGTHMEASURE) [MILLI METRE]
    R = 50.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.000462095287257744 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Volume = 5.97254733286121 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    hoogte workspace = 2570. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Diameter (with insulation) = 360. (IFCLENGTHMEASURE) [MILLI METRE]
    Diameter (without insulation) = 303. (IFCLENGTHMEASURE) [MILLI METRE]
    Height (with insulation) = 2070. (IFCLENGTHMEASURE) [MILLI METRE]
    Height (without insulation) = 2013. (IFCLENGTHMEASURE) [MILLI METRE]
    Height Cold Water Inlet = 70. (IFCLENGTHMEASURE) [MILLI METRE]
    Height Warm Water Outlet = 2010. (IFCLENGTHMEASURE) [MILLI METRE]
    Length = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Width = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Workspace = 860. (IFCLENGTHMEASURE) [MILLI METRE]
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Other | properties | on 1 object (1 IFCBUILDING)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "0001" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  General | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    1e Maintenance (check-up) = "3 months after installation" (IFCTEXT)
    2nd Maintenance (general maintenance) = "12 months after installation" (IFCTEXT)
    Maintenance Interval = "12 months" (IFCTEXT)
    Packaging Height = 2150. (IFCLENGTHMEASURE) [MILLI METRE]
    Packaging Length = 780. (IFCLENGTHMEASURE) [MILLI METRE]
    Packaging Width = 780. (IFCLENGTHMEASURE) [MILLI METRE]
    Transport Weight = 201. (IFCREAL)
    Type of Packaging = "Plastic and Wood" (IFCTEXT)
    Warranty on Parts = "12 months" (IFCTEXT)
    Warranty on Tank = "36 months" (IFCTEXT)
  Model Properties | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Empty Weight = 131. (IFCREAL)
    Insulation Thickness = 57. (IFCLENGTHMEASURE) [MILLI METRE]
    Max. Operating Pressure - tank = 304800. (IFCREAL)
    Max. Temperature - tank = 368.15 (IFCREAL)
    Operating Weight = 630. (IFCREAL)
    Storage Capacity - tank = 499. (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Plumbing | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Cold Water Connection R = 0.166666666666667 (IFCREAL)
    Hot / Warm Water Connection R = 0.166666666666667 (IFCREAL)
    T&P Connection Rp = 0.0625 (IFCREAL)